[preset00]
fRating=1.0
fGammaAdj=1.350000
fDecay=0.980000
fVideoEchoZoom=0.999993
fVideoEchoAlpha=0.5
nVideoEchoOrientation=0
nWaveMode=0
bAdditiveWaves=0
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=1
bSolarize=0
bInvert=0
fWaveAlpha=0.001000
fWaveScale=0.411715
fWaveSmoothing=0.9
fWaveParam=-0.180000
fModWaveAlphaStart=0.750000
fModWaveAlphaEnd=0.950000
fWarpAnimSpeed=1.0
fWarpScale=1.0
fZoomExponent=1.0
fShader=1.0
zoom=0.999999
rot=0.0
cx=0.5
cy=0.5
dx=0.0
dy=0.0
warp=0.010000
sx=1.0
sy=1.0
wave_r=0.0
wave_g=0.0
wave_b=0.0
wave_x=0.5
wave_y=0.5
ob_size=0.0
ob_r=0.0
ob_g=0.0
ob_b=0.0
ob_a=0.920000
ib_size=0.0
ib_r=0.0
ib_g=0.0
ib_b=0.0
ib_a=0.0
nMotionVectorsX=12.0
nMotionVectorsY=9.0
mv_dx=0.0
mv_dy=0.0
mv_l=0.9
mv_r=1.0
mv_g=1.0
mv_b=1.0
mv_a=0.0
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=1
wavecode_0_scaling=0.999998
wavecode_0_smoothing=0.0
wavecode_0_r=0.5
wavecode_0_g=0.6
wavecode_0_b=0.9
wavecode_0_a=1.0
wave_0_per_frame1=a=.3;
wave_0_per_frame2=
wave_0_per_frame3=t1=sin(q5);
wave_0_per_frame4=t2=cos(q5);
wave_0_per_frame5=t3=sin(q6);
wave_0_per_frame6=t4=cos(q6);
wave_0_per_frame7=
wave_0_per_point1=ax=q4*(-1+2*sample);
wave_0_per_point2=ay=q2;
wave_0_per_point3=coef=sqrt(sin(3.1415*sample));
wave_0_per_point4=az=q3+q4*(rand(10000)*.0001)*coef;
wave_0_per_point5=
wave_0_per_point6=ay=ay+.03*q4*sin(q4*.5*ax+q4*.75*(az-q3)+2*time+sin(q4*1.25*ax+q4*.75*(az-q3)+3*time));
wave_0_per_point7=dist=sqrt( sqr(ax)+sqr(az-q3) );
wave_0_per_point8=ay=ay+.05*sin(q4*2.5*dist-3.1415*time);
wave_0_per_point9=
wave_0_per_point10=tcx=q4*(-1+.3333*(q7+.5));
wave_0_per_point11=tcz=q3+q4*(-1+.3333*(q8+.5));
wave_0_per_point12=dist=sqrt( sqr(ax-tcx)+sqr(az-tcz) );
wave_0_per_point13=sw=below(dist,.5*q4)*pow( (1-dist/(.5*q4)),8);
wave_0_per_point14=ay=ay-q4*sw*pow(q1,3);
wave_0_per_point15=a=a+sqrt(q1*sw);
wave_0_per_point16=
wave_0_per_point17=ox = ax*t2 - (az-q3)*t1;
wave_0_per_point18=oy=ay;
wave_0_per_point19=oz = q3 + ax*t1 + (az-q3)*t2;
wave_0_per_point20=
wave_0_per_point21=az=q3+(oz-q3)*t4-(oy-q2)*t3;
wave_0_per_point22=ay=q2+(oz-q3)*t3+(oy-q2)*t4;
wave_0_per_point23=ax=ox;
wave_0_per_point24=
wave_0_per_point25=invz=1/(az+100);
wave_0_per_point26=x=.5+5*ax*invz;
wave_0_per_point27=y=.5+5*ay*invz;
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=1
wavecode_1_scaling=0.999998
wavecode_1_smoothing=0.0
wavecode_1_r=0.5
wavecode_1_g=0.6
wavecode_1_b=0.9
wavecode_1_a=1.0
wave_1_per_frame1=a=.3;
wave_1_per_frame2=
wave_1_per_frame3=t1=sin(q5);
wave_1_per_frame4=t2=cos(q5);
wave_1_per_frame5=t3=sin(q6);
wave_1_per_frame6=t4=cos(q6);
wave_1_per_frame7=
wave_1_per_point1=ax=q4*(-1+2*sample);
wave_1_per_point2=ay=q2;
wave_1_per_point3=coef=sqrt(sin(3.1415*sample));
wave_1_per_point4=az=q3+q4*(-rand(10000)*.0001)*coef;
wave_1_per_point5=
wave_1_per_point6=ay=ay+.03*q4*sin(q4*.5*ax+q4*.75*(az-q3)+2*time+sin(q4*1.25*ax+q4*.75*(az-q3)+3*time));
wave_1_per_point7=dist=sqrt( sqr(ax)+sqr(az-q3) );
wave_1_per_point8=ay=ay+.05*sin(q4*2.5*dist-3.1415*time);
wave_1_per_point9=
wave_1_per_point10=tcx=q4*(-1+.3333*(q7+.5));
wave_1_per_point11=tcz=q3+q4*(-1+.3333*(q8+.5));
wave_1_per_point12=dist=sqrt( sqr(ax-tcx)+sqr(az-tcz) );
wave_1_per_point13=sw=below(dist,.5*q4)*pow( (1-dist/(.5*q4)),8);
wave_1_per_point14=ay=ay-q4*sw*pow(q1,3);
wave_1_per_point15=a=a+sqrt(q1*sw);
wave_1_per_point16=
wave_1_per_point17=ox = ax*t2 - (az-q3)*t1;
wave_1_per_point18=oy=ay;
wave_1_per_point19=oz = q3 + ax*t1 + (az-q3)*t2;
wave_1_per_point20=
wave_1_per_point21=az=q3+(oz-q3)*t4-(oy-q2)*t3;
wave_1_per_point22=ay=q2+(oz-q3)*t3+(oy-q2)*t4;
wave_1_per_point23=ax=ox;
wave_1_per_point24=
wave_1_per_point25=invz=1/(az+100);
wave_1_per_point26=x=.5+5*ax*invz;
wave_1_per_point27=y=.5+5*ay*invz;
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=0
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=1
wavecode_2_scaling=0.999998
wavecode_2_smoothing=0.0
wavecode_2_r=0.4
wavecode_2_g=0.4
wavecode_2_b=0.650000
wavecode_2_a=1.0
wave_2_per_frame1=t1=32;  // double num of rays
wave_2_per_frame2=
wave_2_per_frame3=t5=6.2831*(.08*time-int(.08*time)); //speed
wave_2_per_frame4=t8=0;
wave_2_per_frame5=
wave_2_per_frame6=
wave_2_per_frame7=t3=-1+q7*.3333+.1667;
wave_2_per_frame8=t4=-1+q8*.3333+.1667;
wave_2_per_frame9=
wave_2_per_frame10=t6=pow( q1,3); // interpolation parameter
wave_2_per_frame11=
wave_2_per_frame12=t2=sin(q5);
wave_2_per_frame13=t7=cos(q5);
wave_2_per_point1=sample=.5*sample;
wave_2_per_point2=
wave_2_per_point3=ns=equal(t8%t1,0);
wave_2_per_point4=
wave_2_per_point5=ccx = .85*sin(5.234+100*sample+t5)*cos(200*6.2831*sample+ 3.14*sample+2.45+t5);
wave_2_per_point6=ccy = 1.5*sin(100*sample+0.456+t5)*sin(100*6.2831*sample+ 3.14*sample+1.12+t5);
wave_2_per_point7=ccz = .85*sin(3.12+100*sample+t5)*cos(300*6.2831*sample +3.14*sample+.95+t5);
wave_2_per_point8=
wave_2_per_point9=rr=.075+.067*abs(sin(6.2831*ccy));
wave_2_per_point10=ccx=ccx*(1-t6)+ (t3+rr*cos(sample*6.2831+4*time))*t6;
wave_2_per_point11=ccz=ccz*(1-t6)+ (t4+rr*sin(sample*6.2831+4*time))*t6;
wave_2_per_point12=
wave_2_per_point13=cenx=(1-ns)*cenx+ns*(q4*ccx);
wave_2_per_point14=ceny=(1-ns)*ceny+ns*(q2+q4*abs(ccy));
wave_2_per_point15=cenz=(1-ns)*cenz+ns*(q3+q4*ccz);
wave_2_per_point16=central=equal(t8%2,0);
wave_2_per_point17=angle=6.2831*(t8-1)/t1;
wave_2_per_point18=
wave_2_per_point19=ax=cenx+(1-central)*q4*.02*q4*cos(angle+.12*ceny);
wave_2_per_point20=ay=ceny+(1-central)*q4*.02*q4*sin(angle+.12*ceny);
wave_2_per_point21=az=cenz;
wave_2_per_point22=a=central*above(t8,0)*.07;
wave_2_per_point23=
wave_2_per_point24=ox = cenx+(ax-cenx)*t7+(az-cenz)*t2;
wave_2_per_point25=oy=ay;
wave_2_per_point26=oz = cenz+(ax-cenx)*-t2+(az-cenz)*t7;
wave_2_per_point27=
wave_2_per_point28=ax=ox*t7-(oz-q3)*t2;
wave_2_per_point29=ay=oy;
wave_2_per_point30=az=q3+ox*t2+(oz-q3)*t7;
wave_2_per_point31=
wave_2_per_point32=oz=q3+(az-q3)*cos(q6)-(ay-q2)*sin(q6);
wave_2_per_point33=oy=q2+(az-q3)*sin(q6)+(ay-q2)*cos(q6);
wave_2_per_point34=ox=ax;
wave_2_per_point35=
wave_2_per_point36=invz=1/(oz+100);
wave_2_per_point37=x=.5+5*ox*invz;
wave_2_per_point38=y=.5+5*oy*invz;
wave_2_per_point39=
wave_2_per_point40=t8=(t8+1)%t1;
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=1
wavecode_3_scaling=0.999998
wavecode_3_smoothing=0.0
wavecode_3_r=0.4
wavecode_3_g=0.4
wavecode_3_b=0.650000
wavecode_3_a=1.0
wave_3_per_frame1=t1=32;  // double num of rays
wave_3_per_frame2=
wave_3_per_frame3=t5=6.2831*(.08*time-int(.08*time)); //speed
wave_3_per_frame4=t8=0;
wave_3_per_frame5=
wave_3_per_frame6=
wave_3_per_frame7=t3=-1+q7*.3333+.1667;
wave_3_per_frame8=t4=-1+q8*.3333+.1667;
wave_3_per_frame9=
wave_3_per_frame10=t6=pow( q1,3); // interpolation parameter
wave_3_per_frame11=
wave_3_per_frame12=t2=sin(q5);
wave_3_per_frame13=t7=cos(q5);
wave_3_per_point1=sample=.5*(1+sample);
wave_3_per_point2=
wave_3_per_point3=ns=equal(t8%t1,0);
wave_3_per_point4=
wave_3_per_point5=ccx = .85*sin(5.234+100*sample+t5)*cos(200*6.2831*sample+ 3.14*sample+2.45+t5);
wave_3_per_point6=ccy = 1.5*sin(100*sample+0.456+t5)*sin(100*6.2831*sample+ 3.14*sample+1.12+t5);
wave_3_per_point7=ccz = .85*sin(3.12+100*sample+t5)*cos(300*6.2831*sample +3.14*sample+.95+t5);
wave_3_per_point8=
wave_3_per_point9=rr=.075+.067*abs(sin(6.2831*ccy));
wave_3_per_point10=ccx=ccx*(1-t6)+ (t3+rr*cos(sample*6.2831+4*time))*t6;
wave_3_per_point11=ccz=ccz*(1-t6)+ (t4+rr*sin(sample*6.2831+4*time))*t6;
wave_3_per_point12=
wave_3_per_point13=cenx=(1-ns)*cenx+ns*(q4*ccx);
wave_3_per_point14=ceny=(1-ns)*ceny+ns*(q2+q4*abs(ccy));
wave_3_per_point15=cenz=(1-ns)*cenz+ns*(q3+q4*ccz);
wave_3_per_point16=central=equal(t8%2,0);
wave_3_per_point17=angle=6.2831*(t8-1)/t1;
wave_3_per_point18=
wave_3_per_point19=ax=cenx+(1-central)*q4*.02*q4*cos(angle+.12*ceny);
wave_3_per_point20=ay=ceny+(1-central)*q4*.02*q4*sin(angle+.12*ceny);
wave_3_per_point21=az=cenz;
wave_3_per_point22=a=central*above(t8,0)*.07;
wave_3_per_point23=
wave_3_per_point24=ox = cenx+(ax-cenx)*t7+(az-cenz)*t2;
wave_3_per_point25=oy=ay;
wave_3_per_point26=oz = cenz+(ax-cenx)*-t2+(az-cenz)*t7;
wave_3_per_point27=
wave_3_per_point28=ax=ox*t7-(oz-q3)*t2;
wave_3_per_point29=ay=oy;
wave_3_per_point30=az=q3+ox*t2+(oz-q3)*t7;
wave_3_per_point31=
wave_3_per_point32=oz=q3+(az-q3)*cos(q6)-(ay-q2)*sin(q6);
wave_3_per_point33=oy=q2+(az-q3)*sin(q6)+(ay-q2)*cos(q6);
wave_3_per_point34=ox=ax;
wave_3_per_point35=
wave_3_per_point36=invz=1/(oz+100);
wave_3_per_point37=x=.5+5*ox*invz;
wave_3_per_point38=y=.5+5*oy*invz;
wave_3_per_point39=
wave_3_per_point40=t8=(t8+1)%t1;
shapecode_0_enabled=0
shapecode_0_sides=30
shapecode_0_additive=1
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_x=0.5
shapecode_0_y=0.5
shapecode_0_rad=0.042497
shapecode_0_ang=0.0
shapecode_0_tex_ang=0.0
shapecode_0_tex_zoom=1.0
shapecode_0_r=0.8
shapecode_0_g=0.1
shapecode_0_b=0.8
shapecode_0_a=1.0
shapecode_0_r2=0.0
shapecode_0_g2=0.0
shapecode_0_b2=0.0
shapecode_0_a2=0.0
shapecode_0_border_r=1.0
shapecode_0_border_g=1.0
shapecode_0_border_b=1.0
shapecode_0_border_a=0.0
shapecode_1_enabled=0
shapecode_1_sides=30
shapecode_1_additive=1
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_x=0.5
shapecode_1_y=0.5
shapecode_1_rad=0.042077
shapecode_1_ang=0.0
shapecode_1_tex_ang=0.0
shapecode_1_tex_zoom=0.999998
shapecode_1_r=1.0
shapecode_1_g=0.3
shapecode_1_b=0.1
shapecode_1_a=1.0
shapecode_1_r2=0.0
shapecode_1_g2=0.0
shapecode_1_b2=0.0
shapecode_1_a2=0.0
shapecode_1_border_r=1.0
shapecode_1_border_g=1.0
shapecode_1_border_b=1.0
shapecode_1_border_a=0.0
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_x=0.5
shapecode_2_y=0.5
shapecode_2_rad=0.1
shapecode_2_ang=0.0
shapecode_2_tex_ang=0.0
shapecode_2_tex_zoom=1.0
shapecode_2_r=1.0
shapecode_2_g=0.0
shapecode_2_b=0.0
shapecode_2_a=1.0
shapecode_2_r2=0.0
shapecode_2_g2=1.0
shapecode_2_b2=0.0
shapecode_2_a2=0.0
shapecode_2_border_r=1.0
shapecode_2_border_g=1.0
shapecode_2_border_b=1.0
shapecode_2_border_a=0.1
shapecode_3_enabled=1
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_x=0.5
shapecode_3_y=0.5
shapecode_3_rad=1.978841
shapecode_3_ang=0.0
shapecode_3_tex_ang=0.0
shapecode_3_tex_zoom=0.344203
shapecode_3_r=0.0
shapecode_3_g=0.0
shapecode_3_b=0.0
shapecode_3_a=0.0
shapecode_3_r2=1.0
shapecode_3_g2=1.0
shapecode_3_b2=1.0
shapecode_3_a2=0.0
shapecode_3_border_r=1.0
shapecode_3_border_g=1.0
shapecode_3_border_b=1.0
shapecode_3_border_a=0.0
per_frame_1=warp=0;
per_frame_2=zoom=1;
per_frame_3=
per_frame_4=rnd=equal(frame%400,0);
per_frame_5=offy=(1-rnd)*offy+rnd*(-3+rand(600)/100);
per_frame_6=offz=(1-rnd)*offz+rnd*(-80-0*rand(1000)/1000);
per_frame_7=sc=(1-rnd)*sc+rnd*(1+rand(500)/100);
per_frame_8=offx=0;
per_frame_9=offy=-3.1;
per_frame_10=offz=-60;
per_frame_11=sc=4;
per_frame_12=
per_frame_13=q2=offy; // y-offset
per_frame_14=q3=offz; // z-offset
per_frame_15=q4=sc; // scale
per_frame_16=
per_frame_17=q5=3.1415*cos(.05*time+.84+sin(time*.1+6.43)); // rot-y;
per_frame_18=q6=.25+.2*sin(time*.15+2.43+cos(time*.09+1.87)); // rot-x;
per_frame_19=
per_frame_20=
per_frame_21=stime=if(equal(stime,0),time,stime );
per_frame_22=mytime=time-stime;
per_frame_23=phase = .1*mytime - int(.1*mytime);
per_frame_24=tilex=if(below(phase,.025),1 + rand(4),tilex );
per_frame_25=tilez=if(below(phase,.025),1 + rand(4),tilez );
per_frame_26=q7=tilex;
per_frame_27=q8=tilez;
per_frame_28=q1=abs(sin(3.1415*phase));
per_frame_29=
per_frame_30=echo_zoom=1.007;
