[preset00]
fRating=3.000000
fGammaAdj=1.000000
fDecay=0.500000
fVideoEchoZoom=1.006596
fVideoEchoAlpha=0.000000
nVideoEchoOrientation=3
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=4.099998
fWaveScale=1.285751
fWaveSmoothing=0.630000
fWaveParam=0.000000
fModWaveAlphaStart=0.710000
fModWaveAlphaEnd=1.300000
fWarpAnimSpeed=1.000000
fWarpScale=1.331000
fZoomExponent=1.000000
fShader=0.000000
zoom=0.999514
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.010000
sx=1.000000
sy=1.000000
wave_r=0.650000
wave_g=0.650000
wave_b=0.650000
wave_x=0.500000
wave_y=0.500000
ob_size=0.500000
ob_r=0.010000
ob_g=0.000000
ob_b=0.000000
ob_a=0.000000
ib_size=0.260000
ib_r=0.250000
ib_g=0.250000
ib_b=0.250000
ib_a=0.000000
nMotionVectorsX=12.000000
nMotionVectorsY=9.000000
mv_dx=0.000000
mv_dy=0.000000
mv_l=0.900000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=0.000000
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=1
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=0
wavecode_0_bAdditive=0
wavecode_0_scaling=1.000000
wavecode_0_smoothing=0.000000
wavecode_0_r=1.000000
wavecode_0_g=1.000000
wavecode_0_b=1.000000
wavecode_0_a=1.000000
wave_0_per_frame1=vol = (bass_att + mid_att + treb_att)*.333333;
wave_0_per_frame2=vol_avg = .1*(vol_avg*9 + vol);
wave_0_per_frame3=vg = vol_avg*.1;
wave_0_per_frame4=t1 = if(above(vg,1.8),1.8,vg);
wave_0_per_point1=tm = q1;
wave_0_per_point2=sp = sample*6.28*8*6;
wave_0_per_point3=
wave_0_per_point4=vol = (value1+value2)*.5;
wave_0_per_point5=it = it*above(sample,0);
wave_0_per_point6=it = it + 1;
wave_0_per_point7=rad = .5 + vol + .03;
wave_0_per_point8=ra = rad*sin(sample*3.14);
wave_0_per_point9=ox = ra*sin(sp);
wave_0_per_point10=oy = sin(sample*3.14-1.57)*rad;
wave_0_per_point11=oz = ra*cos(sp);
wave_0_per_point12=
wave_0_per_point13=xang = tm*.132;
wave_0_per_point14=sxang = 0;
wave_0_per_point15=yang = tm*.153;
wave_0_per_point16=ayang = 0;
wave_0_per_point17=zang = tm*.110;
wave_0_per_point18=azang = 0;
wave_0_per_point19=fov = 0.6 + 0.2*sin(tm);
wave_0_per_point20=fov = .5;
wave_0_per_point21=
wave_0_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_0_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_0_per_point24=ox = mx;
wave_0_per_point25=oy = my;
wave_0_per_point26=mx = ox*cos(yang) + oz*sin(yang);
wave_0_per_point27=mz = - ox*sin(yang) + oz*cos(yang);
wave_0_per_point28=ox = mx;
wave_0_per_point29=oz = mz;
wave_0_per_point30=my = oy*cos(xang) - oz*sin(xang);
wave_0_per_point31=mz = oy*sin(xang) + oz*cos(xang);
wave_0_per_point32=oy = my;
wave_0_per_point33=oz = mz;
wave_0_per_point34=
wave_0_per_point35=oz = oz - 2;
wave_0_per_point36=x = ox*fov/oz + 0.5;
wave_0_per_point37=x = (x-.5)*0.75 + 0.5;
wave_0_per_point38=y = oy*fov/oz + 0.5;
wave_0_per_point39=
wave_0_per_point40=r = 1;
wave_0_per_point41=g = .25+.25*sin(sp);
wave_0_per_point42=b = 0;
wave_0_per_point43=a = .5 + (oz+2)*.5;
wave_0_per_point44=a = a*below(z,2);
wave_0_per_point45=minrgb = min(r,min(g,b));
wave_0_per_point46=maxrgb = max(r,max(g,b));
wave_0_per_point47=l = (maxrgb-minrgb)*.5;
wave_0_per_point48=diff = maxrgb-minrgb;
wave_0_per_point49=sum = maxrgb+minrgb;
wave_0_per_point50=s = if(above(l,0.5),diff/(2-sum),diff/sum)*(1-equal(l,0));
wave_0_per_point51=h = if(equal(r,maxrgb),(g-b)/diff,if(equal(g,maxrgb),2+(b-r)/diff,4+(r-g)/diff));
wave_0_per_point52=h = h*0.1666666;
wave_0_per_point53=h = if(below(h,0),0,if(above(h,1),1,h));
wave_0_per_point54=
wave_0_per_point55=h = h + time*0.05*1.324 +.15;
wave_0_per_point56=h = h - int(h);
wave_0_per_point57=
wave_0_per_point58=tmpb = if(below(l,0.5),l*(1+s),(l+s)-(s*l));
wave_0_per_point59=tmpa = 2*l - tmpb;
wave_0_per_point60=hvr = h + .333333;
wave_0_per_point61=hvr = if(below(hvr,0),hvr+1,if(above(hvr,1),hvr-1,hvr));
wave_0_per_point62=hvg = h;
wave_0_per_point63=hvg = if(below(hvg,0),hvg+1,if(above(hvg,1),hvg-1,hvg));
wave_0_per_point64=hvb = h - .333333;
wave_0_per_point65=hvb = if(below(hvb,0),hvb+1,if(above(hvb,1),hvb-1,hvb));
wave_0_per_point66=
wave_0_per_point67=r = if(below(6*hvr,1),tmpa+(tmpb-tmpa)*6*hvr, if(below(2*hvr,1),tmpb, if(below(hvr*3,2),tmpa+(tmpb-tmpa)*(.666666-hvr)*6,tmpa)));
wave_0_per_point68=g = if(below(6*hvg,1),tmpa+(tmpb-tmpa)*6*hvg, if(below(2*hvg,1),tmpb, if(below(hvg*3,2),tmpa+(tmpb-tmpa)*(.666666-hvg)*6,tmpa)));
wave_0_per_point69=b = if(below(6*hvb,1),tmpa+(tmpb-tmpa)*6*hvb, if(below(2*hvb,1),tmpb, if(below(hvb*3,2),tmpa+(tmpb-tmpa)*(.666666-hvb)*6,tmpa)));
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=1
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=0
wavecode_1_scaling=1.000000
wavecode_1_smoothing=0.000000
wavecode_1_r=1.000000
wavecode_1_g=1.000000
wavecode_1_b=1.000000
wavecode_1_a=1.000000
wave_1_per_frame1=vol = (bass_att + mid_att + treb_att)*.333333;
wave_1_per_frame2=vol_avg = .1*(vol_avg*9 + vol);
wave_1_per_frame3=vg = vol_avg*.1;
wave_1_per_frame4=t1 = if(above(vg,1.8),1.8,vg);
wave_1_per_point1=tm = q1;
wave_1_per_point2=sp = sample*6.28*8*6;
wave_1_per_point3=
wave_1_per_point4=vol = (value1+value2)*.5;
wave_1_per_point5=it = it*above(sample,0);
wave_1_per_point6=it = it + 1;
wave_1_per_point7=rad = .5 + vol + .02;
wave_1_per_point8=ra = rad*sin(sample*3.14);
wave_1_per_point9=ox = ra*sin(sp);
wave_1_per_point10=oy = sin(sample*3.14-1.57)*rad;
wave_1_per_point11=oz = ra*cos(sp);
wave_1_per_point12=
wave_1_per_point13=xang = tm*.132;
wave_1_per_point14=sxang = 0;
wave_1_per_point15=yang = tm*.153;
wave_1_per_point16=ayang = 0;
wave_1_per_point17=zang = tm*.110;
wave_1_per_point18=azang = 0;
wave_1_per_point19=fov = 0.6 + 0.2*sin(tm);
wave_1_per_point20=fov = .5;
wave_1_per_point21=
wave_1_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_1_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_1_per_point24=ox = mx;
wave_1_per_point25=oy = my;
wave_1_per_point26=mx = ox*cos(yang) + oz*sin(yang);
wave_1_per_point27=mz = - ox*sin(yang) + oz*cos(yang);
wave_1_per_point28=ox = mx;
wave_1_per_point29=oz = mz;
wave_1_per_point30=my = oy*cos(xang) - oz*sin(xang);
wave_1_per_point31=mz = oy*sin(xang) + oz*cos(xang);
wave_1_per_point32=oy = my;
wave_1_per_point33=oz = mz;
wave_1_per_point34=
wave_1_per_point35=oz = oz - 2;
wave_1_per_point36=x = ox*fov/oz + 0.5;
wave_1_per_point37=x = (x-.5)*0.75 + 0.5;
wave_1_per_point38=y = oy*fov/oz + 0.5;
wave_1_per_point39=
wave_1_per_point40=r = 1;
wave_1_per_point41=g = .25+.25*sin(sp);
wave_1_per_point42=b = 0;
wave_1_per_point43=a = .5 + (oz+2)*.5;
wave_1_per_point44=a = a*below(z,2);
wave_1_per_point45=minrgb = min(r,min(g,b));
wave_1_per_point46=maxrgb = max(r,max(g,b));
wave_1_per_point47=l = (maxrgb-minrgb)*.5;
wave_1_per_point48=diff = maxrgb-minrgb;
wave_1_per_point49=sum = maxrgb+minrgb;
wave_1_per_point50=s = if(above(l,0.5),diff/(2-sum),diff/sum)*(1-equal(l,0));
wave_1_per_point51=h = if(equal(r,maxrgb),(g-b)/diff,if(equal(g,maxrgb),2+(b-r)/diff,4+(r-g)/diff));
wave_1_per_point52=h = h*0.1666666;
wave_1_per_point53=h = if(below(h,0),0,if(above(h,1),1,h));
wave_1_per_point54=
wave_1_per_point55=h = h + time*0.05*1.324 + .1;
wave_1_per_point56=h = h - int(h);
wave_1_per_point57=
wave_1_per_point58=tmpb = if(below(l,0.5),l*(1+s),(l+s)-(s*l));
wave_1_per_point59=tmpa = 2*l - tmpb;
wave_1_per_point60=hvr = h + .333333;
wave_1_per_point61=hvr = if(below(hvr,0),hvr+1,if(above(hvr,1),hvr-1,hvr));
wave_1_per_point62=hvg = h;
wave_1_per_point63=hvg = if(below(hvg,0),hvg+1,if(above(hvg,1),hvg-1,hvg));
wave_1_per_point64=hvb = h - .333333;
wave_1_per_point65=hvb = if(below(hvb,0),hvb+1,if(above(hvb,1),hvb-1,hvb));
wave_1_per_point66=
wave_1_per_point67=r = if(below(6*hvr,1),tmpa+(tmpb-tmpa)*6*hvr, if(below(2*hvr,1),tmpb, if(below(hvr*3,2),tmpa+(tmpb-tmpa)*(.666666-hvr)*6,tmpa)));
wave_1_per_point68=g = if(below(6*hvg,1),tmpa+(tmpb-tmpa)*6*hvg, if(below(2*hvg,1),tmpb, if(below(hvg*3,2),tmpa+(tmpb-tmpa)*(.666666-hvg)*6,tmpa)));
wave_1_per_point69=b = if(below(6*hvb,1),tmpa+(tmpb-tmpa)*6*hvb, if(below(2*hvb,1),tmpb, if(below(hvb*3,2),tmpa+(tmpb-tmpa)*(.666666-hvb)*6,tmpa)));
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=1
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.000000
wavecode_2_smoothing=0.000000
wavecode_2_r=1.000000
wavecode_2_g=1.000000
wavecode_2_b=1.000000
wavecode_2_a=1.000000
wave_2_per_frame1=vol = (bass_att + mid_att + treb_att)*.333333;
wave_2_per_frame2=vol_avg = .1*(vol_avg*9 + vol);
wave_2_per_frame3=vg = vol_avg*.1;
wave_2_per_frame4=t1 = if(above(vg,1.8),1.8,vg);
wave_2_per_point1=tm = q1;
wave_2_per_point2=sp = sample*6.28*8*6;
wave_2_per_point3=
wave_2_per_point4=vol = (value1+value2)*.5;
wave_2_per_point5=it = it*above(sample,0);
wave_2_per_point6=it = it + 1;
wave_2_per_point7=rad = .5 + vol + .01;
wave_2_per_point8=ra = rad*sin(sample*3.14);
wave_2_per_point9=ox = ra*sin(sp);
wave_2_per_point10=oy = sin(sample*3.14-1.57)*rad;
wave_2_per_point11=oz = ra*cos(sp);
wave_2_per_point12=
wave_2_per_point13=xang = tm*.132;
wave_2_per_point14=sxang = 0;
wave_2_per_point15=yang = tm*.153;
wave_2_per_point16=ayang = 0;
wave_2_per_point17=zang = tm*.110;
wave_2_per_point18=azang = 0;
wave_2_per_point19=fov = 0.6 + 0.2*sin(tm);
wave_2_per_point20=fov = .5;
wave_2_per_point21=
wave_2_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_2_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_2_per_point24=ox = mx;
wave_2_per_point25=oy = my;
wave_2_per_point26=mx = ox*cos(yang) + oz*sin(yang);
wave_2_per_point27=mz = - ox*sin(yang) + oz*cos(yang);
wave_2_per_point28=ox = mx;
wave_2_per_point29=oz = mz;
wave_2_per_point30=my = oy*cos(xang) - oz*sin(xang);
wave_2_per_point31=mz = oy*sin(xang) + oz*cos(xang);
wave_2_per_point32=oy = my;
wave_2_per_point33=oz = mz;
wave_2_per_point34=
wave_2_per_point35=oz = oz - 2;
wave_2_per_point36=x = ox*fov/oz + 0.5;
wave_2_per_point37=x = (x-.5)*0.75 + 0.5;
wave_2_per_point38=y = oy*fov/oz + 0.5;
wave_2_per_point39=
wave_2_per_point40=r = 1;
wave_2_per_point41=g = .25+.25*sin(sp);
wave_2_per_point42=b = 0;
wave_2_per_point43=a = .5 + (oz+2)*.5;
wave_2_per_point44=a = a*below(z,2);
wave_2_per_point45=minrgb = min(r,min(g,b));
wave_2_per_point46=maxrgb = max(r,max(g,b));
wave_2_per_point47=l = (maxrgb-minrgb)*.5;
wave_2_per_point48=diff = maxrgb-minrgb;
wave_2_per_point49=sum = maxrgb+minrgb;
wave_2_per_point50=s = if(above(l,0.5),diff/(2-sum),diff/sum)*(1-equal(l,0));
wave_2_per_point51=h = if(equal(r,maxrgb),(g-b)/diff,if(equal(g,maxrgb),2+(b-r)/diff,4+(r-g)/diff));
wave_2_per_point52=h = h*0.1666666;
wave_2_per_point53=h = if(below(h,0),0,if(above(h,1),1,h));
wave_2_per_point54=
wave_2_per_point55=h = h + time*0.05*1.324 + .05;
wave_2_per_point56=h = h - int(h);
wave_2_per_point57=
wave_2_per_point58=tmpb = if(below(l,0.5),l*(1+s),(l+s)-(s*l));
wave_2_per_point59=tmpa = 2*l - tmpb;
wave_2_per_point60=hvr = h + .333333;
wave_2_per_point61=hvr = if(below(hvr,0),hvr+1,if(above(hvr,1),hvr-1,hvr));
wave_2_per_point62=hvg = h;
wave_2_per_point63=hvg = if(below(hvg,0),hvg+1,if(above(hvg,1),hvg-1,hvg));
wave_2_per_point64=hvb = h - .333333;
wave_2_per_point65=hvb = if(below(hvb,0),hvb+1,if(above(hvb,1),hvb-1,hvb));
wave_2_per_point66=
wave_2_per_point67=r = if(below(6*hvr,1),tmpa+(tmpb-tmpa)*6*hvr, if(below(2*hvr,1),tmpb, if(below(hvr*3,2),tmpa+(tmpb-tmpa)*(.666666-hvr)*6,tmpa)));
wave_2_per_point68=g = if(below(6*hvg,1),tmpa+(tmpb-tmpa)*6*hvg, if(below(2*hvg,1),tmpb, if(below(hvg*3,2),tmpa+(tmpb-tmpa)*(.666666-hvg)*6,tmpa)));
wave_2_per_point69=b = if(below(6*hvb,1),tmpa+(tmpb-tmpa)*6*hvb, if(below(2*hvb,1),tmpb, if(below(hvb*3,2),tmpa+(tmpb-tmpa)*(.666666-hvb)*6,tmpa)));
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=1
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=0
wavecode_3_scaling=1.000000
wavecode_3_smoothing=0.000000
wavecode_3_r=1.000000
wavecode_3_g=1.000000
wavecode_3_b=1.000000
wavecode_3_a=1.000000
wave_3_per_frame1=vol = (bass_att + mid_att + treb_att)*.333333;
wave_3_per_frame2=vol_avg = .1*(vol_avg*9 + vol);
wave_3_per_frame3=vg = vol_avg*.1;
wave_3_per_frame4=t1 = if(above(vg,1.8),1.8,vg);
wave_3_per_point1=tm = q1;
wave_3_per_point2=sp = sample*6.28*8*6;
wave_3_per_point3=
wave_3_per_point4=vol = (value1+value2)*.5;
wave_3_per_point5=it = it*above(sample,0);
wave_3_per_point6=it = it + 1;
wave_3_per_point7=rad = .5 + vol;
wave_3_per_point8=ra = rad*sin(sample*3.14);
wave_3_per_point9=ox = ra*sin(sp);
wave_3_per_point10=oy = sin(sample*3.14-1.57)*rad;
wave_3_per_point11=oz = ra*cos(sp);
wave_3_per_point12=
wave_3_per_point13=xang = tm*.132;
wave_3_per_point14=sxang = 0;
wave_3_per_point15=yang = tm*.153;
wave_3_per_point16=ayang = 0;
wave_3_per_point17=zang = tm*.110;
wave_3_per_point18=azang = 0;
wave_3_per_point19=fov = 0.6 + 0.2*sin(tm);
wave_3_per_point20=fov = .5;
wave_3_per_point21=
wave_3_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_3_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_3_per_point24=ox = mx;
wave_3_per_point25=oy = my;
wave_3_per_point26=mx = ox*cos(yang) + oz*sin(yang);
wave_3_per_point27=mz = - ox*sin(yang) + oz*cos(yang);
wave_3_per_point28=ox = mx;
wave_3_per_point29=oz = mz;
wave_3_per_point30=my = oy*cos(xang) - oz*sin(xang);
wave_3_per_point31=mz = oy*sin(xang) + oz*cos(xang);
wave_3_per_point32=oy = my;
wave_3_per_point33=oz = mz;
wave_3_per_point34=
wave_3_per_point35=oz = oz - 2;
wave_3_per_point36=x = ox*fov/oz + 0.5;
wave_3_per_point37=x = (x-.5)*0.75 + 0.5;
wave_3_per_point38=y = oy*fov/oz + 0.5;
wave_3_per_point39=
wave_3_per_point40=r = 1;
wave_3_per_point41=g = .25+.25*sin(sp);
wave_3_per_point42=b = 0;
wave_3_per_point43=a = .5 + (oz+2)*.5;
wave_3_per_point44=a = a*below(z,2);
wave_3_per_point45=minrgb = min(r,min(g,b));
wave_3_per_point46=maxrgb = max(r,max(g,b));
wave_3_per_point47=l = (maxrgb-minrgb)*.5;
wave_3_per_point48=diff = maxrgb-minrgb;
wave_3_per_point49=sum = maxrgb+minrgb;
wave_3_per_point50=s = if(above(l,0.5),diff/(2-sum),diff/sum)*(1-equal(l,0));
wave_3_per_point51=h = if(equal(r,maxrgb),(g-b)/diff,if(equal(g,maxrgb),2+(b-r)/diff,4+(r-g)/diff));
wave_3_per_point52=h = h*0.1666666;
wave_3_per_point53=h = if(below(h,0),0,if(above(h,1),1,h));
wave_3_per_point54=
wave_3_per_point55=h = h + time*0.05*1.324;
wave_3_per_point56=h = h - int(h);
wave_3_per_point57=
wave_3_per_point58=tmpb = if(below(l,0.5),l*(1+s),(l+s)-(s*l));
wave_3_per_point59=tmpa = 2*l - tmpb;
wave_3_per_point60=hvr = h + .333333;
wave_3_per_point61=hvr = if(below(hvr,0),hvr+1,if(above(hvr,1),hvr-1,hvr));
wave_3_per_point62=hvg = h;
wave_3_per_point63=hvg = if(below(hvg,0),hvg+1,if(above(hvg,1),hvg-1,hvg));
wave_3_per_point64=hvb = h - .333333;
wave_3_per_point65=hvb = if(below(hvb,0),hvb+1,if(above(hvb,1),hvb-1,hvb));
wave_3_per_point66=
wave_3_per_point67=r = if(below(6*hvr,1),tmpa+(tmpb-tmpa)*6*hvr, if(below(2*hvr,1),tmpb, if(below(hvr*3,2),tmpa+(tmpb-tmpa)*(.666666-hvr)*6,tmpa)));
wave_3_per_point68=g = if(below(6*hvg,1),tmpa+(tmpb-tmpa)*6*hvg, if(below(2*hvg,1),tmpb, if(below(hvg*3,2),tmpa+(tmpb-tmpa)*(.666666-hvg)*6,tmpa)));
wave_3_per_point69=b = if(below(6*hvb,1),tmpa+(tmpb-tmpa)*6*hvb, if(below(2*hvb,1),tmpb, if(below(hvb*3,2),tmpa+(tmpb-tmpa)*(.666666-hvb)*6,tmpa)));
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_x=0.500000
shapecode_0_y=0.500000
shapecode_0_rad=0.100000
shapecode_0_ang=0.000000
shapecode_0_tex_ang=0.000000
shapecode_0_tex_zoom=1.000000
shapecode_0_r=1.000000
shapecode_0_g=0.000000
shapecode_0_b=0.000000
shapecode_0_a=1.000000
shapecode_0_r2=0.000000
shapecode_0_g2=1.000000
shapecode_0_b2=0.000000
shapecode_0_a2=0.000000
shapecode_0_border_r=1.000000
shapecode_0_border_g=1.000000
shapecode_0_border_b=1.000000
shapecode_0_border_a=0.100000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_x=0.500000
shapecode_1_y=0.500000
shapecode_1_rad=0.100000
shapecode_1_ang=0.000000
shapecode_1_tex_ang=0.000000
shapecode_1_tex_zoom=1.000000
shapecode_1_r=1.000000
shapecode_1_g=0.000000
shapecode_1_b=0.000000
shapecode_1_a=1.000000
shapecode_1_r2=0.000000
shapecode_1_g2=1.000000
shapecode_1_b2=0.000000
shapecode_1_a2=0.000000
shapecode_1_border_r=1.000000
shapecode_1_border_g=1.000000
shapecode_1_border_b=1.000000
shapecode_1_border_a=0.100000
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_x=0.500000
shapecode_2_y=0.500000
shapecode_2_rad=0.100000
shapecode_2_ang=0.000000
shapecode_2_tex_ang=0.000000
shapecode_2_tex_zoom=1.000000
shapecode_2_r=1.000000
shapecode_2_g=0.000000
shapecode_2_b=0.000000
shapecode_2_a=1.000000
shapecode_2_r2=0.000000
shapecode_2_g2=1.000000
shapecode_2_b2=0.000000
shapecode_2_a2=0.000000
shapecode_2_border_r=1.000000
shapecode_2_border_g=1.000000
shapecode_2_border_b=1.000000
shapecode_2_border_a=0.100000
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_x=0.500000
shapecode_3_y=0.500000
shapecode_3_rad=0.100000
shapecode_3_ang=0.000000
shapecode_3_tex_ang=0.000000
shapecode_3_tex_zoom=1.000000
shapecode_3_r=1.000000
shapecode_3_g=0.000000
shapecode_3_b=0.000000
shapecode_3_a=1.000000
shapecode_3_r2=0.000000
shapecode_3_g2=1.000000
shapecode_3_b2=0.000000
shapecode_3_a2=0.000000
shapecode_3_border_r=1.000000
shapecode_3_border_g=1.000000
shapecode_3_border_b=1.000000
shapecode_3_border_a=0.100000
per_frame_1=wave_a = 0;
per_frame_2=
per_frame_3=vol = (bass_att + treb_att + mid_att)*.333333;
per_frame_4=
per_frame_5=tic = time-tin;
per_frame_6=tin = time;
per_frame_7=tm = tm + tic*vol;
per_frame_8=q1 = tm;
