[preset00]
fRating=3.000000
fGammaAdj=1.700000
fDecay=1.000000
fVideoEchoZoom=0.999600
fVideoEchoAlpha=0.500000
nVideoEchoOrientation=1
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=1
bDarken=1
bSolarize=0
bInvert=1
fWaveAlpha=0.001000
fWaveScale=1.285751
fWaveSmoothing=0.630000
fWaveParam=0.000000
fModWaveAlphaStart=0.710000
fModWaveAlphaEnd=1.300000
fWarpAnimSpeed=1.000000
fWarpScale=1.331000
fZoomExponent=1.000000
fShader=0.000000
zoom=0.999514
rot=0.000001
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.010000
sx=0.999999
sy=1.115500
wave_r=0.650000
wave_g=0.650000
wave_b=0.650000
wave_x=0.500000
wave_y=0.500000
ob_size=0.500000
ob_r=0.010000
ob_g=0.000000
ob_b=0.000000
ob_a=0.000000
ib_size=0.260000
ib_r=0.250000
ib_g=0.250000
ib_b=0.250000
ib_a=0.000000
nMotionVectorsX=2.560000
nMotionVectorsY=48.000000
mv_dx=0.360000
mv_dy=-0.800000
mv_l=5.000000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=0.000000
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=1.000000
wavecode_0_smoothing=0.800000
wavecode_0_r=1.000000
wavecode_0_g=1.000000
wavecode_0_b=1.000000
wavecode_0_a=1.000000
wave_0_per_point1=sw = (1-sw)*above(sample,0);
wave_0_per_point2=
wave_0_per_point3=osa = sample*above(sample,0);
wave_0_per_point4=
wave_0_per_point5=mod = pow(value1*2,2)*sign(value1)*.5;
wave_0_per_point6=
wave_0_per_point7=mod = value1;
wave_0_per_point8=mod = mod*sw;
wave_0_per_point9=
wave_0_per_point10=x = if(sw,osa,sample);
wave_0_per_point11=x = sample*.5;
wave_0_per_point12=y = 1 + mod*.5;
wave_0_per_point13=
wave_0_per_point14=osa = sample;
wave_0_per_point15=
wave_0_per_point16=mo = 3.7 + mod*6 + q1;
wave_0_per_point17=
wave_0_per_point18=r = .5 + sin(mo)*.5;
wave_0_per_point19=g = .5 + sin(mo + 1.0472)*.5;
wave_0_per_point20=b = .5 + sin(mo + 2.0944)*.5;
wave_0_per_point21=
wave_0_per_point22=a = 1 - abs(mod)*12;
wave_0_per_point23=a = 1-sw;
wave_0_per_point24=a = max(0,min(a,1));
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=1.000000
wavecode_1_smoothing=0.800000
wavecode_1_r=1.000000
wavecode_1_g=1.000000
wavecode_1_b=1.000000
wavecode_1_a=1.000000
wave_1_per_point1=sw = (1-sw)*below(sample,1);
wave_1_per_point2=
wave_1_per_point3=osa = sample*above(sample,0);
wave_1_per_point4=
wave_1_per_point5=mod = pow(value1*2,2)*sign(value1)*.5;
wave_1_per_point6=
wave_1_per_point7=mod = value1;
wave_1_per_point8=mod = mod*sw;
wave_1_per_point9=
wave_1_per_point10=x = if(sw,osa,sample);
wave_1_per_point11=x = 1-sample*.5;
wave_1_per_point12=y = 0 + mod*.5;
wave_1_per_point13=
wave_1_per_point14=osa = sample;
wave_1_per_point15=
wave_1_per_point16=mo = 3.7 + mod*6 + q1;
wave_1_per_point17=
wave_1_per_point18=r = .5 + sin(mo)*.5;
wave_1_per_point19=g = .5 + sin(mo + 1.0472)*.5;
wave_1_per_point20=b = .5 + sin(mo + 2.0944)*.5;
wave_1_per_point21=
wave_1_per_point22=a = 1 - abs(mod)*12;
wave_1_per_point23=a = 1-sw;
wave_1_per_point24=a = max(0,min(a,1));
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=0
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.000000
wavecode_2_smoothing=0.800000
wavecode_2_r=0.000000
wavecode_2_g=0.000000
wavecode_2_b=0.000000
wavecode_2_a=1.000000
wave_2_per_point1=sw = (1-sw)*above(sample,0);
wave_2_per_point2=
wave_2_per_point3=osa = sample*above(sample,0);
wave_2_per_point4=
wave_2_per_point5=mod = pow(value1*2,2)*sign(value1)*.5;
wave_2_per_point6=
wave_2_per_point7=mod = value1;
wave_2_per_point8=mod = mod;
wave_2_per_point9=
wave_2_per_point10=x = if(sw,osa,sample);
wave_2_per_point11=x = sample*.5;
wave_2_per_point12=y = 1 + mod*.5;
wave_2_per_point13=
wave_2_per_point14=osa = sample;
wave_2_per_point15=
wave_2_per_point16=mo = 3.7 + mod*6 + q1;
wave_2_per_point17=
wave_2_per_point18=//r = .5 + sin(mo)*.5;
wave_2_per_point19=//g = .5 + sin(mo + 1.0472)*.5;
wave_2_per_point20=//b = .5 + sin(mo + 2.0944)*.5;
wave_2_per_point21=
wave_2_per_point22=//a = 1 - abs(mod)*12;
wave_2_per_point23=//a = 1-sw;
wave_2_per_point24=a = max(0,min(a,1));
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=0
wavecode_3_scaling=1.000000
wavecode_3_smoothing=0.800000
wavecode_3_r=0.000000
wavecode_3_g=0.000000
wavecode_3_b=0.000000
wavecode_3_a=1.000000
wave_3_per_point1=sw = (1-sw)*above(sample,0);
wave_3_per_point2=
wave_3_per_point3=osa = sample*above(sample,0);
wave_3_per_point4=
wave_3_per_point5=mod = pow(value1*2,2)*sign(value1)*.5;
wave_3_per_point6=
wave_3_per_point7=mod = value1;
wave_3_per_point8=mod = mod;
wave_3_per_point9=
wave_3_per_point10=x = if(sw,osa,sample);
wave_3_per_point11=x = 1 - sample*.5;
wave_3_per_point12=y = 0 + mod*.5;
wave_3_per_point13=
wave_3_per_point14=osa = sample;
wave_3_per_point15=
wave_3_per_point16=mo = 3.7 + mod*6 + q1;
wave_3_per_point17=
wave_3_per_point18=//r = .5 + sin(mo)*.5;
wave_3_per_point19=//g = .5 + sin(mo + 1.0472)*.5;
wave_3_per_point20=//b = .5 + sin(mo + 2.0944)*.5;
wave_3_per_point21=
wave_3_per_point22=//a = 1 - abs(mod)*12;
wave_3_per_point23=//a = 1-sw;
wave_3_per_point24=a = max(0,min(a,1));
shapecode_0_enabled=1
shapecode_0_sides=54
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_x=0.500000
shapecode_0_y=1.000000
shapecode_0_rad=0.134785
shapecode_0_ang=0.000000
shapecode_0_tex_ang=0.000000
shapecode_0_tex_zoom=1.000000
shapecode_0_r=0.000000
shapecode_0_g=0.000000
shapecode_0_b=0.000000
shapecode_0_a=1.000000
shapecode_0_r2=0.000000
shapecode_0_g2=0.000000
shapecode_0_b2=0.000000
shapecode_0_a2=0.000000
shapecode_0_border_r=1.000000
shapecode_0_border_g=1.000000
shapecode_0_border_b=1.000000
shapecode_0_border_a=0.000000
shape_0_per_frame1=ti = q1;
shape_0_per_frame2=rad = q2;
shape_0_per_frame3=x = (ti - int(ti))*.5;
shape_0_per_frame4=
shape_0_per_frame5=
shapecode_1_enabled=1
shapecode_1_sides=54
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_x=0.500000
shapecode_1_y=0.000000
shapecode_1_rad=0.134785
shapecode_1_ang=0.000000
shapecode_1_tex_ang=0.000000
shapecode_1_tex_zoom=1.000000
shapecode_1_r=0.000000
shapecode_1_g=0.000000
shapecode_1_b=0.000000
shapecode_1_a=1.000000
shapecode_1_r2=0.000000
shapecode_1_g2=0.000000
shapecode_1_b2=0.000000
shapecode_1_a2=0.000000
shapecode_1_border_r=1.000000
shapecode_1_border_g=1.000000
shapecode_1_border_b=1.000000
shapecode_1_border_a=0.000000
shape_1_per_frame1=ti = q1;
shape_1_per_frame2=rad = q2;
shape_1_per_frame3=x = 1-(ti - int(ti))*.5;
shape_1_per_frame4=
shapecode_2_enabled=1
shapecode_2_sides=43
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=1
shapecode_2_x=0.690000
shapecode_2_y=0.500000
shapecode_2_rad=0.548200
shapecode_2_ang=0.000000
shapecode_2_tex_ang=3.895574
shapecode_2_tex_zoom=1.000000
shapecode_2_r=1.000000
shapecode_2_g=1.000000
shapecode_2_b=1.000000
shapecode_2_a=1.000000
shapecode_2_r2=1.000000
shapecode_2_g2=1.000000
shapecode_2_b2=1.000000
shapecode_2_a2=1.000000
shapecode_2_border_r=1.000000
shapecode_2_border_g=0.000000
shapecode_2_border_b=1.000000
shapecode_2_border_a=0.000000
shape_2_per_frame1=rad = .4 + q3;
shape_2_per_frame2=
shape_2_per_frame3=tex_zoom = 1/rad*.8;
shape_2_per_frame4=
shape_2_per_frame5=x = .5 + q3;
shape_2_per_frame6=
shape_2_per_frame7=tex_ang = -q4;
shape_2_per_frame8=
shape_2_per_frame9=ti = q5 + sin(time*1.234);
shape_2_per_frame10=
shape_2_per_frame11=x = .5 + q3*sin(ti);
shape_2_per_frame12=y = .5 + q3*cos(ti)*.5;
shapecode_3_enabled=1
shapecode_3_sides=43
shapecode_3_additive=0
shapecode_3_thickOutline=1
shapecode_3_textured=1
shapecode_3_x=0.500001
shapecode_3_y=0.500000
shapecode_3_rad=0.548218
shapecode_3_ang=0.000000
shapecode_3_tex_ang=0.879646
shapecode_3_tex_zoom=1.000000
shapecode_3_r=1.000000
shapecode_3_g=1.000000
shapecode_3_b=1.000000
shapecode_3_a=1.000000
shapecode_3_r2=1.000000
shapecode_3_g2=1.000000
shapecode_3_b2=1.000000
shapecode_3_a2=1.000000
shapecode_3_border_r=1.000000
shapecode_3_border_g=1.000000
shapecode_3_border_b=1.000000
shapecode_3_border_a=0.000000
shape_3_per_frame1=rad = .4 + q3;
shape_3_per_frame2=
shape_3_per_frame3=tex_zoom = 1/rad*.8;
shape_3_per_frame4=
shape_3_per_frame5=x = .5 - q3;
shape_3_per_frame6=
shape_3_per_frame7=tex_ang = q4;
shape_3_per_frame8=
shape_3_per_frame9=ti = q5 + sin(time*.948) + 3.1416;
shape_3_per_frame10=
shape_3_per_frame11=x = .5 + q3*sin(ti)*1.5;
shape_3_per_frame12=y = .5 + q3*cos(ti)*.5;
per_frame_1=warp = 0;
per_frame_2=
per_frame_3=tic = min(time-tin,.1);
per_frame_4=tin = time;
per_frame_5=
per_frame_6=vol = (bass_att + treb_att + mid_att)*.333333;
per_frame_7=
per_frame_8=ra = 1/tic*.25;
per_frame_9=
per_frame_10=vav = tic*(vav*(1/tic - ra) + ra*(bass+treb+mid)*.33333);
per_frame_11=
per_frame_12=ra = 1/tic*.05;
per_frame_13=treb_avg = tic*(treb_avg*(1/tic - ra) + ra*treb);
per_frame_14=mid_avg = tic*(mid_avg*(1/tic - ra) + ra*mid);
per_frame_15=
per_frame_16=ra = 1/tic*.1;
per_frame_17=bass_avg = tic*(bass_avg*(1/tic - ra) + ra*bass);
per_frame_18=
per_frame_19=
per_frame_20=tt = tt + tic*treb;
per_frame_21=mt = mt + tic*mid;
per_frame_22=bt = bt + tic*bass;
per_frame_23=vt = vt + tic*vav;
per_frame_24=
per_frame_25=q1 = time;
per_frame_26=
per_frame_27=q2 = vav*.1;
per_frame_28=
per_frame_29=q3 = .02 + bass_avg*.05;
per_frame_30=q4 = .5 + (treb_avg + mid_avg)*.25;
per_frame_31=//q4 = (treb_avg - mid_avg);
per_frame_32=//q4 = bass_avg - (treb_avg + mid_avg)*.5;
per_frame_33=//q4 = -bass_avg;
per_frame_34=
per_frame_35=
per_frame_36=q5 = vt*3;
per_frame_37=
per_frame_38=monitor = q4;
per_frame_39=
per_frame_40=//rot = .025*max(.7,vav);
per_frame_41=rot = .025*(.7 + vav*.25);
per_frame_42=//rot = .025*vav;
per_frame_43=
per_pixel_1=mod = .1;
per_pixel_2=
per_pixel_3=//sw = above(x,.5);
per_pixel_4=
per_pixel_5=//dy = mod*pow(abs(y - .5)*2,1.5)*sign(y-.5);
per_pixel_6=
per_pixel_7=//dy = .2*sign(y-.5)*sw;
per_pixel_8=
per_pixel_9=//sy = 1 + (1-sw)*.116;
per_pixel_10=
per_pixel_11=
per_pixel_12=//rot = .05;
per_pixel_13=
per_pixel_14=cx = if(above(y,.5),-1,2);
