[preset00]
fRating=2.000000
fGammaAdj=1.980000
fDecay=0.500000
fVideoEchoZoom=0.999608
fVideoEchoAlpha=0.000000
nVideoEchoOrientation=3
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=4.099998
fWaveScale=1.285751
fWaveSmoothing=0.630000
fWaveParam=0.000000
fModWaveAlphaStart=0.710000
fModWaveAlphaEnd=1.300000
fWarpAnimSpeed=1.000000
fWarpScale=1.331000
fZoomExponent=1.868310
fShader=0.000000
zoom=1.000195
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.010000
sx=1.000000
sy=1.000000
wave_r=0.650000
wave_g=0.650000
wave_b=0.650000
wave_x=0.500000
wave_y=0.500000
ob_size=0.005000
ob_r=0.000000
ob_g=0.000000
ob_b=0.000000
ob_a=1.000000
ib_size=0.260000
ib_r=0.250000
ib_g=0.250000
ib_b=0.250000
ib_a=0.000000
nMotionVectorsX=12.000000
nMotionVectorsY=9.000000
mv_dx=0.000000
mv_dy=0.000000
mv_l=0.900000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=0.000000
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=1
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=0
wavecode_0_bAdditive=1
wavecode_0_scaling=1.000000
wavecode_0_smoothing=0.000000
wavecode_0_r=0.700000
wavecode_0_g=0.900000
wavecode_0_b=1.000000
wavecode_0_a=1.000000
wave_0_per_frame1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_0_per_frame2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_0_per_frame3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_0_per_frame4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_0_per_frame5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_0_per_frame6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_0_per_frame7=
wave_0_per_frame8=t1 = ra*6.2832;
wave_0_per_frame9=t2 = rb*6.2832;
wave_0_per_frame10=t3 = rc*6.2832;
wave_0_per_frame11=t4 = rd*6.2832;
wave_0_per_frame12=t5 = re*6.2832;
wave_0_per_frame13=t6 = rf*6.2832;
wave_0_per_frame14=
wave_0_per_frame15=rg = if(rg,rg,.1 + .8*rand(1001)*.001);
wave_0_per_frame16=rh = if(rh,rh,.1 + .8*rand(1001)*.001);
wave_0_per_frame17=
wave_0_per_frame18=t7 = rg;
wave_0_per_frame19=t8 = rh;
wave_0_per_frame20=
wave_0_per_point1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_0_per_point2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_0_per_point3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_0_per_point4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_0_per_point5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_0_per_point6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_0_per_point7=rg = if(rg,rg,2 + 8*rand(1001)*.001);
wave_0_per_point8=rh = if(rh,rh,2 + 8*rand(1001)*.001);
wave_0_per_point9=ri = if(ri,ri,2 + 8*rand(1001)*.001);
wave_0_per_point10=rj = if(rj,rj,2 + 8*rand(1001)*.001);
wave_0_per_point11=rk = if(rk,rk,2 + 8*rand(1001)*.001);
wave_0_per_point12=rl = if(rl,rl,2 + 8*rand(1001)*.001);
wave_0_per_point13=rm = if(rm,rm,2 + 8*rand(1001)*.001);
wave_0_per_point14=rn = if(rn,rn,2 + 8*rand(1001)*.001);
wave_0_per_point15=ro = if(ro,ro,2 + 8*rand(1001)*.001);
wave_0_per_point16=rp = if(rp,rp,2 + 8*rand(1001)*.001);
wave_0_per_point17=rq = if(rq,rq,2 + 8*rand(1001)*.001);
wave_0_per_point18=rr = if(rr,rr,2 + 8*rand(1001)*.001);
wave_0_per_point19=
wave_0_per_point20=it = it*above(sample,0);
wave_0_per_point21=it = it + 1;
wave_0_per_point22=pi = 6.2813;
wave_0_per_point23=
wave_0_per_point24=sam = sample;
wave_0_per_point25=a = min((1-sam)*value2*3,1);
wave_0_per_point26=b = 1;
wave_0_per_point27=r = pow(1 - sam,2);
wave_0_per_point28=g = pow(1 - sam,.4);
wave_0_per_point29=
wave_0_per_point30=sp = q1*.05 - sam*.2;
wave_0_per_point31=spa = q2*.05 - sam*.2;
wave_0_per_point32=spb = q3*.05 - sam*.2;
wave_0_per_point33=ox = sam*(.5*sin(sp*ra*pi) + .5*sin(sp*rd*pi));
wave_0_per_point34=oy = sam*(.5*sin(sp*rb*pi) + .5*sin(sp*re*pi));
wave_0_per_point35=oz = sam*(.5*sin(sp*rc*pi) + .5*sin(sp*rf*pi));
wave_0_per_point36=
wave_0_per_point37=cut = .2;
wave_0_per_point38=sam = sam*above(sam,cut);
wave_0_per_point39=mo = rand(2);
wave_0_per_point40=ox = ox + max(0,sam-cut)*if(mo,sin(spa*rg),sin(spa*rh));
wave_0_per_point41=oy = oy + max(0,sam-cut)*if(mo,sin(spa*ri),sin(spa*rj));
wave_0_per_point42=oz = oz + max(0,sam-cut)*if(mo,sin(spa*rk),sin(spa*rl));
wave_0_per_point43=
wave_0_per_point44=cut = .4;
wave_0_per_point45=sam = sam*above(sam,cut);
wave_0_per_point46=mo = rand(2);
wave_0_per_point47=ox = ox + max(0,sam-cut)*if(mo,sin(spb*rm),sin(spb*rp));
wave_0_per_point48=oy = oy + max(0,sam-cut)*if(mo,sin(spb*rn),sin(spb*rq));
wave_0_per_point49=oz = oz + max(0,sam-cut)*if(mo,sin(spb*ro),sin(spb*rr));
wave_0_per_point50=
wave_0_per_point51=
wave_0_per_point52=xang = q1*.1;
wave_0_per_point53=yang = q2*.1;
wave_0_per_point54=zang = q3*.1;
wave_0_per_point55=
wave_0_per_point56=fov = .5;
wave_0_per_point57=
wave_0_per_point58=mx = ox*cos(yang) + oz*sin(yang);
wave_0_per_point59=mz = - ox*sin(yang) + oz*cos(yang);
wave_0_per_point60=ox = mx;
wave_0_per_point61=oz = mz;
wave_0_per_point62=mx = ox*cos(zang) - oy*sin(zang);
wave_0_per_point63=my = ox*sin(zang) + oy*cos(zang);
wave_0_per_point64=ox = mx;
wave_0_per_point65=oy = my;
wave_0_per_point66=my = oy*cos(xang) - oz*sin(xang);
wave_0_per_point67=mz = oy*sin(xang) + oz*cos(xang);
wave_0_per_point68=oy = my;
wave_0_per_point69=oz = mz;
wave_0_per_point70=
wave_0_per_point71=
wave_0_per_point72=ox = ox*q4;
wave_0_per_point73=oy = oy*q4;
wave_0_per_point74=oz = oz*q4;
wave_0_per_point75=
wave_0_per_point76=oz = oz - 2;
wave_0_per_point77=x = ox*fov/oz + 0.5;
wave_0_per_point78=x = (x-.5)*0.75 + 0.5;
wave_0_per_point79=y = oy*fov/oz + 0.5;
wave_0_per_point80=
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=1
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=1
wavecode_1_scaling=1.000000
wavecode_1_smoothing=0.000000
wavecode_1_r=0.700000
wavecode_1_g=0.900000
wavecode_1_b=1.000000
wavecode_1_a=1.000000
wave_1_per_frame1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_1_per_frame2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_1_per_frame3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_1_per_frame4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_1_per_frame5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_1_per_frame6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_1_per_frame7=
wave_1_per_frame8=t1 = ra*6.2832;
wave_1_per_frame9=t2 = rb*6.2832;
wave_1_per_frame10=t3 = rc*6.2832;
wave_1_per_frame11=t4 = rd*6.2832;
wave_1_per_frame12=t5 = re*6.2832;
wave_1_per_frame13=t6 = rf*6.2832;
wave_1_per_frame14=
wave_1_per_frame15=rg = if(rg,rg,.1 + .8*rand(1001)*.001);
wave_1_per_frame16=rh = if(rh,rh,.1 + .8*rand(1001)*.001);
wave_1_per_frame17=
wave_1_per_frame18=t7 = rg;
wave_1_per_frame19=t8 = rh;
wave_1_per_frame20=
wave_1_per_point1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_1_per_point2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_1_per_point3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_1_per_point4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_1_per_point5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_1_per_point6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_1_per_point7=rg = if(rg,rg,2 + 8*rand(1001)*.001);
wave_1_per_point8=rh = if(rh,rh,2 + 8*rand(1001)*.001);
wave_1_per_point9=ri = if(ri,ri,2 + 8*rand(1001)*.001);
wave_1_per_point10=rj = if(rj,rj,2 + 8*rand(1001)*.001);
wave_1_per_point11=rk = if(rk,rk,2 + 8*rand(1001)*.001);
wave_1_per_point12=rl = if(rl,rl,2 + 8*rand(1001)*.001);
wave_1_per_point13=rm = if(rm,rm,2 + 8*rand(1001)*.001);
wave_1_per_point14=rn = if(rn,rn,2 + 8*rand(1001)*.001);
wave_1_per_point15=ro = if(ro,ro,2 + 8*rand(1001)*.001);
wave_1_per_point16=rp = if(rp,rp,2 + 8*rand(1001)*.001);
wave_1_per_point17=rq = if(rq,rq,2 + 8*rand(1001)*.001);
wave_1_per_point18=rr = if(rr,rr,2 + 8*rand(1001)*.001);
wave_1_per_point19=
wave_1_per_point20=it = it*above(sample,0);
wave_1_per_point21=it = it + 1;
wave_1_per_point22=pi = 6.2813;
wave_1_per_point23=
wave_1_per_point24=sam = sample;
wave_1_per_point25=a = min((1-sam)*value2*3,1);
wave_1_per_point26=b = 1;
wave_1_per_point27=r = pow(1 - sam,2);
wave_1_per_point28=g = pow(1 - sam,.4);
wave_1_per_point29=
wave_1_per_point30=sp = q1*.05 - sam*.2;
wave_1_per_point31=spa = q2*.05 - sam*.2;
wave_1_per_point32=spb = q3*.05 - sam*.2;
wave_1_per_point33=ox = sam*(.5*sin(sp*ra*pi) + .5*sin(sp*rd*pi));
wave_1_per_point34=oy = sam*(.5*sin(sp*rb*pi) + .5*sin(sp*re*pi));
wave_1_per_point35=oz = sam*(.5*sin(sp*rc*pi) + .5*sin(sp*rf*pi));
wave_1_per_point36=
wave_1_per_point37=cut = .2;
wave_1_per_point38=sam = sam*above(sam,cut);
wave_1_per_point39=mo = rand(2);
wave_1_per_point40=ox = ox + max(0,sam-cut)*if(mo,sin(spa*rg),sin(spa*rh));
wave_1_per_point41=oy = oy + max(0,sam-cut)*if(mo,sin(spa*ri),sin(spa*rj));
wave_1_per_point42=oz = oz + max(0,sam-cut)*if(mo,sin(spa*rk),sin(spa*rl));
wave_1_per_point43=
wave_1_per_point44=cut = .4;
wave_1_per_point45=sam = sam*above(sam,cut);
wave_1_per_point46=mo = rand(2);
wave_1_per_point47=ox = ox + max(0,sam-cut)*if(mo,sin(spb*rm),sin(spb*rp));
wave_1_per_point48=oy = oy + max(0,sam-cut)*if(mo,sin(spb*rn),sin(spb*rq));
wave_1_per_point49=oz = oz + max(0,sam-cut)*if(mo,sin(spb*ro),sin(spb*rr));
wave_1_per_point50=
wave_1_per_point51=
wave_1_per_point52=xang = q1*.1;
wave_1_per_point53=yang = q2*.1;
wave_1_per_point54=zang = q3*.1;
wave_1_per_point55=
wave_1_per_point56=fov = .5;
wave_1_per_point57=
wave_1_per_point58=mx = ox*cos(yang) + oz*sin(yang);
wave_1_per_point59=mz = - ox*sin(yang) + oz*cos(yang);
wave_1_per_point60=ox = mx;
wave_1_per_point61=oz = mz;
wave_1_per_point62=mx = ox*cos(zang) - oy*sin(zang);
wave_1_per_point63=my = ox*sin(zang) + oy*cos(zang);
wave_1_per_point64=ox = mx;
wave_1_per_point65=oy = my;
wave_1_per_point66=my = oy*cos(xang) - oz*sin(xang);
wave_1_per_point67=mz = oy*sin(xang) + oz*cos(xang);
wave_1_per_point68=oy = my;
wave_1_per_point69=oz = mz;
wave_1_per_point70=
wave_1_per_point71=
wave_1_per_point72=ox = ox*q4;
wave_1_per_point73=oy = oy*q4;
wave_1_per_point74=oz = oz*q4;
wave_1_per_point75=
wave_1_per_point76=oz = oz - 2;
wave_1_per_point77=x = ox*fov/oz + 0.5;
wave_1_per_point78=x = (x-.5)*0.75 + 0.5;
wave_1_per_point79=y = oy*fov/oz + 0.5;
wave_1_per_point80=
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=1
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=0
wavecode_2_bAdditive=1
wavecode_2_scaling=1.000000
wavecode_2_smoothing=0.000000
wavecode_2_r=0.700000
wavecode_2_g=0.900000
wavecode_2_b=1.000000
wavecode_2_a=1.000000
wave_2_per_frame1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_2_per_frame2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_2_per_frame3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_2_per_frame4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_2_per_frame5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_2_per_frame6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_2_per_frame7=
wave_2_per_frame8=t1 = ra*6.2832;
wave_2_per_frame9=t2 = rb*6.2832;
wave_2_per_frame10=t3 = rc*6.2832;
wave_2_per_frame11=t4 = rd*6.2832;
wave_2_per_frame12=t5 = re*6.2832;
wave_2_per_frame13=t6 = rf*6.2832;
wave_2_per_frame14=
wave_2_per_frame15=rg = if(rg,rg,.1 + .8*rand(1001)*.001);
wave_2_per_frame16=rh = if(rh,rh,.1 + .8*rand(1001)*.001);
wave_2_per_frame17=
wave_2_per_frame18=t7 = rg;
wave_2_per_frame19=t8 = rh;
wave_2_per_frame20=
wave_2_per_point1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_2_per_point2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_2_per_point3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_2_per_point4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_2_per_point5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_2_per_point6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_2_per_point7=rg = if(rg,rg,2 + 8*rand(1001)*.001);
wave_2_per_point8=rh = if(rh,rh,2 + 8*rand(1001)*.001);
wave_2_per_point9=ri = if(ri,ri,2 + 8*rand(1001)*.001);
wave_2_per_point10=rj = if(rj,rj,2 + 8*rand(1001)*.001);
wave_2_per_point11=rk = if(rk,rk,2 + 8*rand(1001)*.001);
wave_2_per_point12=rl = if(rl,rl,2 + 8*rand(1001)*.001);
wave_2_per_point13=rm = if(rm,rm,2 + 8*rand(1001)*.001);
wave_2_per_point14=rn = if(rn,rn,2 + 8*rand(1001)*.001);
wave_2_per_point15=ro = if(ro,ro,2 + 8*rand(1001)*.001);
wave_2_per_point16=rp = if(rp,rp,2 + 8*rand(1001)*.001);
wave_2_per_point17=rq = if(rq,rq,2 + 8*rand(1001)*.001);
wave_2_per_point18=rr = if(rr,rr,2 + 8*rand(1001)*.001);
wave_2_per_point19=
wave_2_per_point20=it = it*above(sample,0);
wave_2_per_point21=it = it + 1;
wave_2_per_point22=pi = 6.2813;
wave_2_per_point23=
wave_2_per_point24=sam = sample;
wave_2_per_point25=a = min((1-sam)*value2*3,1);
wave_2_per_point26=b = 1;
wave_2_per_point27=r = pow(1 - sam,2);
wave_2_per_point28=g = pow(1 - sam,.4);
wave_2_per_point29=
wave_2_per_point30=sp = q1*.05 - sam*.2;
wave_2_per_point31=spa = q2*.05 - sam*.2;
wave_2_per_point32=spb = q3*.05 - sam*.2;
wave_2_per_point33=ox = sam*(.5*sin(sp*ra*pi) + .5*sin(sp*rd*pi));
wave_2_per_point34=oy = sam*(.5*sin(sp*rb*pi) + .5*sin(sp*re*pi));
wave_2_per_point35=oz = sam*(.5*sin(sp*rc*pi) + .5*sin(sp*rf*pi));
wave_2_per_point36=
wave_2_per_point37=cut = .2;
wave_2_per_point38=sam = sam*above(sam,cut);
wave_2_per_point39=mo = rand(2);
wave_2_per_point40=ox = ox + max(0,sam-cut)*if(mo,sin(spa*rg),sin(spa*rh));
wave_2_per_point41=oy = oy + max(0,sam-cut)*if(mo,sin(spa*ri),sin(spa*rj));
wave_2_per_point42=oz = oz + max(0,sam-cut)*if(mo,sin(spa*rk),sin(spa*rl));
wave_2_per_point43=
wave_2_per_point44=cut = .4;
wave_2_per_point45=sam = sam*above(sam,cut);
wave_2_per_point46=mo = rand(2);
wave_2_per_point47=ox = ox + max(0,sam-cut)*if(mo,sin(spb*rm),sin(spb*rp));
wave_2_per_point48=oy = oy + max(0,sam-cut)*if(mo,sin(spb*rn),sin(spb*rq));
wave_2_per_point49=oz = oz + max(0,sam-cut)*if(mo,sin(spb*ro),sin(spb*rr));
wave_2_per_point50=
wave_2_per_point51=
wave_2_per_point52=xang = q1*.1;
wave_2_per_point53=yang = q2*.1;
wave_2_per_point54=zang = q3*.1;
wave_2_per_point55=
wave_2_per_point56=fov = .5;
wave_2_per_point57=
wave_2_per_point58=mx = ox*cos(yang) + oz*sin(yang);
wave_2_per_point59=mz = - ox*sin(yang) + oz*cos(yang);
wave_2_per_point60=ox = mx;
wave_2_per_point61=oz = mz;
wave_2_per_point62=mx = ox*cos(zang) - oy*sin(zang);
wave_2_per_point63=my = ox*sin(zang) + oy*cos(zang);
wave_2_per_point64=ox = mx;
wave_2_per_point65=oy = my;
wave_2_per_point66=my = oy*cos(xang) - oz*sin(xang);
wave_2_per_point67=mz = oy*sin(xang) + oz*cos(xang);
wave_2_per_point68=oy = my;
wave_2_per_point69=oz = mz;
wave_2_per_point70=
wave_2_per_point71=
wave_2_per_point72=ox = ox*q4;
wave_2_per_point73=oy = oy*q4;
wave_2_per_point74=oz = oz*q4;
wave_2_per_point75=
wave_2_per_point76=oz = oz - 2;
wave_2_per_point77=x = ox*fov/oz + 0.5;
wave_2_per_point78=x = (x-.5)*0.75 + 0.5;
wave_2_per_point79=y = oy*fov/oz + 0.5;
wave_2_per_point80=
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=1
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=0
wavecode_3_bAdditive=0
wavecode_3_scaling=1.000000
wavecode_3_smoothing=0.000000
wavecode_3_r=1.000000
wavecode_3_g=1.000000
wavecode_3_b=1.000000
wavecode_3_a=0.400000
wave_3_per_point1=sp = sample*10;
wave_3_per_point2=ti = q5*2;
wave_3_per_point3=
wave_3_per_point4=ox = .25*sin(ti*.327 + sp*6.2832*3.12) + .5*sin(ti*.878 + sp*6.2832*8.68) + .25*sin(ti*.787 + sp*6.2832*7.85);
wave_3_per_point5=oy = .45*sin(ti*.877 + sp*6.2832*2.37) + .25*sin(ti*.482 + sp*6.2832*2.38) + .3*sin(ti*.129 + sp*6.2832*3.21);
wave_3_per_point6=oz = .35*sin(ti*.453 + sp*6.2832*8.97) + .15*sin(ti*.365 + sp*6.2832*5.13) + .5*sin(ti*.385 + sp*6.2832*5.46);
wave_3_per_point7=
wave_3_per_point8=oy = oy + time*.05;
wave_3_per_point9=oy = abs(oy - int(oy*1)*1);
wave_3_per_point10=
wave_3_per_point11=fov = .5;
wave_3_per_point12=
wave_3_per_point13=oy = oy - .5;
wave_3_per_point14=
wave_3_per_point15=oy = oy*20;
wave_3_per_point16=ox = ox*12;
wave_3_per_point17=oz = oz*10;
wave_3_per_point18=
wave_3_per_point19=oz = oz -2;
wave_3_per_point20=
wave_3_per_point21=x = ox*fov/oz + 0.5;
wave_3_per_point22=x = (x-.5)*0.75 + 0.5;
wave_3_per_point23=y = oy*fov/oz + 0.5;
wave_3_per_point24=
wave_3_per_point25=a = a*below(oz,-.1)*(.25 + .75*sample)*.5;
wave_3_per_point26=
wave_3_per_point27=r = .85 + .15*sin(sample*6.28*21.6);
wave_3_per_point28=g = .85 + .15*sin(sample*6.28*18.1);
wave_3_per_point29=b = .85 + .15*sin(sample*6.28*15.8);
wave_3_per_point30=
wave_3_per_point31=
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_x=0.500000
shapecode_0_y=0.500000
shapecode_0_rad=0.100000
shapecode_0_ang=0.000000
shapecode_0_tex_ang=0.000000
shapecode_0_tex_zoom=1.000000
shapecode_0_r=1.000000
shapecode_0_g=0.000000
shapecode_0_b=0.000000
shapecode_0_a=1.000000
shapecode_0_r2=0.000000
shapecode_0_g2=1.000000
shapecode_0_b2=0.000000
shapecode_0_a2=0.000000
shapecode_0_border_r=1.000000
shapecode_0_border_g=1.000000
shapecode_0_border_b=1.000000
shapecode_0_border_a=0.100000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_x=0.500000
shapecode_1_y=0.500000
shapecode_1_rad=0.100000
shapecode_1_ang=0.000000
shapecode_1_tex_ang=0.000000
shapecode_1_tex_zoom=1.000000
shapecode_1_r=1.000000
shapecode_1_g=0.000000
shapecode_1_b=0.000000
shapecode_1_a=1.000000
shapecode_1_r2=0.000000
shapecode_1_g2=1.000000
shapecode_1_b2=0.000000
shapecode_1_a2=0.000000
shapecode_1_border_r=1.000000
shapecode_1_border_g=1.000000
shapecode_1_border_b=1.000000
shapecode_1_border_a=0.100000
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_x=0.500000
shapecode_2_y=0.500000
shapecode_2_rad=0.100000
shapecode_2_ang=0.000000
shapecode_2_tex_ang=0.000000
shapecode_2_tex_zoom=1.000000
shapecode_2_r=1.000000
shapecode_2_g=0.000000
shapecode_2_b=0.000000
shapecode_2_a=1.000000
shapecode_2_r2=0.000000
shapecode_2_g2=1.000000
shapecode_2_b2=0.000000
shapecode_2_a2=0.000000
shapecode_2_border_r=1.000000
shapecode_2_border_g=1.000000
shapecode_2_border_b=1.000000
shapecode_2_border_a=0.100000
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_x=0.500000
shapecode_3_y=0.500000
shapecode_3_rad=0.100000
shapecode_3_ang=0.000000
shapecode_3_tex_ang=0.000000
shapecode_3_tex_zoom=1.000000
shapecode_3_r=1.000000
shapecode_3_g=0.000000
shapecode_3_b=0.000000
shapecode_3_a=1.000000
shapecode_3_r2=0.000000
shapecode_3_g2=1.000000
shapecode_3_b2=0.000000
shapecode_3_a2=0.000000
shapecode_3_border_r=1.000000
shapecode_3_border_g=1.000000
shapecode_3_border_b=1.000000
shapecode_3_border_a=0.100000
per_frame_1=wave_a = 0;
per_frame_2=decay = 0.1;
per_frame_3=
per_frame_4=vol = (bass_att + treb_att + mid_att)*.333333;
per_frame_5=
per_frame_6=tic = min(time-tin,.1);
per_frame_7=tin = time;
per_frame_8=
per_frame_9=ra = 10;
per_frame_10=treb_avg = tic*(treb_avg*(1/tic - ra) + ra*treb);
per_frame_11=mid_avg = tic*(mid_avg*(1/tic - ra) + ra*mid);
per_frame_12=bass_avg = tic*(bass_avg*(1/tic - ra) + ra*bass);
per_frame_13=vav = tic*(vav*(1/tic - ra) + ra*(bass+treb+mid)*.33333);
per_frame_14=
per_frame_15=tt = tt + tic*treb_avg;
per_frame_16=mt = mt + tic*mid_avg;
per_frame_17=bt = bt + tic*bass_avg;
per_frame_18=
per_frame_19=sp = abs(vav - slide)*.1;
per_frame_20=slide = if(above(slide,vav),slide-tic*sp,slide+tic*sp) + (1-toc)*vav;
per_frame_21=toc = 1;
per_frame_22=
per_frame_23=vt = vt + tic*slide;
per_frame_24=
per_frame_25=q1 = bt;
per_frame_26=q2 = mt;
per_frame_27=q3 = tt;
per_frame_28=q4 = slide*1;
per_frame_29=q5 = vt*.05 + 150;
