[preset00]
fRating=3.000000
fGammaAdj=1.280000
fDecay=0.960000
fVideoEchoZoom=0.996627
fVideoEchoAlpha=0.500000
nVideoEchoOrientation=1
nWaveMode=2
bAdditiveWaves=0
bWaveDots=1
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001000
fWaveScale=0.011726
fWaveSmoothing=0.900000
fWaveParam=0.000000
fModWaveAlphaStart=0.750000
fModWaveAlphaEnd=0.950000
fWarpAnimSpeed=0.037492
fWarpScale=0.014889
fZoomExponent=1.000000
fShader=0.000000
zoom=1.000000
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.033004
sx=1.000000
sy=1.000000
wave_r=0.500000
wave_g=0.400000
wave_b=0.300000
wave_x=0.500000
wave_y=0.500000
ob_size=0.005000
ob_r=0.110000
ob_g=1.000000
ob_b=1.000000
ob_a=1.000000
ib_size=0.000000
ib_r=0.000000
ib_g=1.000000
ib_b=1.000000
ib_a=0.000000
nMotionVectorsX=3.000000
nMotionVectorsY=2.000000
mv_dx=0.020000
mv_dy=-0.020000
mv_l=0.150000
mv_r=0.490000
mv_g=0.480000
mv_b=0.300001
mv_a=0.000000
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=1.000000
wavecode_0_smoothing=0.500000
wavecode_0_r=0.100000
wavecode_0_g=1.000000
wavecode_0_b=0.700000
wavecode_0_a=1.000000
wave_0_per_point1=n=sample*6.283;
wave_0_per_point2=phs=-sample * 0.2;
wave_0_per_point3=tm=q1 + phs*4;
wave_0_per_point4=
wave_0_per_point5=flip=flip+1;
wave_0_per_point6=flip=flip*below(flip,2);
wave_0_per_point7=
wave_0_per_point8=xp=0;
wave_0_per_point9=yp=(flip*0.1-0.05)*(1-sample);
wave_0_per_point10=zp=0;
wave_0_per_point11=
wave_0_per_point12=//spin;
wave_0_per_point13=ang=tm*20;
wave_0_per_point14=sa=sin(ang);ca=cos(ang);
wave_0_per_point15=xr=xp*sa + yp*ca;
wave_0_per_point16=yr=xp*ca - yp*sa;
wave_0_per_point17=zr=zp;
wave_0_per_point18=
wave_0_per_point19=xp=xr;
wave_0_per_point20=yp=yr + 0.05 + (sin(tm)*0.5 + 0.5)*0.2 + 0.05;
wave_0_per_point21=zp=zr;
wave_0_per_point22=
wave_0_per_point23=//wrist movement;
wave_0_per_point24=ang=sin(tm*2)*0.5 +0.5;
wave_0_per_point25=
wave_0_per_point26=xq=xp;
wave_0_per_point27=sa=sin(ang);ca=cos(ang);
wave_0_per_point28=yq=yp*sa + zp*ca;
wave_0_per_point29=zq=yp*ca - zp*sa;
wave_0_per_point30=
wave_0_per_point31=
wave_0_per_point32=ang=tm*8;
wave_0_per_point33=sa=sin(ang);ca=cos(ang);
wave_0_per_point34=xp=xq*sa + yq*ca;
wave_0_per_point35=yp=xq*ca - yq*sa;
wave_0_per_point36=zp=zq;
wave_0_per_point37=
wave_0_per_point38=//forearm movement;
wave_0_per_point39=zp=zp-0.3;
wave_0_per_point40=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_0_per_point41=xq=xp;
wave_0_per_point42=sa=sin(ang);ca=cos(ang);
wave_0_per_point43=yq=yp*sa + zp*ca;
wave_0_per_point44=zq=yp*ca - zp*sa;
wave_0_per_point45=
wave_0_per_point46=//upper arm twist
wave_0_per_point47=ang=-1.0 + cos(tm*3 + 0.5);
wave_0_per_point48=xp=xq*sa + yq*ca;
wave_0_per_point49=yp=xq*ca - yq*sa;
wave_0_per_point50=zp=zq;
wave_0_per_point51=
wave_0_per_point52=//upper arm outward;
wave_0_per_point53=zp=zp-0.35;
wave_0_per_point54=ang=cos(tm*2)*0.75 - 1.05;
wave_0_per_point55=sa=sin(ang);ca=cos(ang);
wave_0_per_point56=xq=xp*sa + zp*ca;
wave_0_per_point57=yq=yp;
wave_0_per_point58=zq=xp*ca - zp*sa;
wave_0_per_point59=
wave_0_per_point60=//upper arm up down;
wave_0_per_point61=ang=cos(tm)*0.5 - 0.5;
wave_0_per_point62=xp=xq;
wave_0_per_point63=sa=sin(ang);ca=cos(ang);
wave_0_per_point64=yp=yq*ca - zq*sa;
wave_0_per_point65=zp=yq*sa + zq*ca;
wave_0_per_point66=
wave_0_per_point67=//xp=xq;yp=yq;zp=zq;
wave_0_per_point68=
wave_0_per_point69=
wave_0_per_point70=//project into screenspace and draw on screen
wave_0_per_point71=zp=zp+2;
wave_0_per_point72=xs=xp/zp;
wave_0_per_point73=ys=yp/zp;
wave_0_per_point74=
wave_0_per_point75=x=xs+0.5;
wave_0_per_point76=y=ys*1.3+0.5;
wave_0_per_point77=
wave_0_per_point78=
wave_0_per_point79=a=(1-sample);
wave_0_per_point80=
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=1.000000
wavecode_1_smoothing=0.500000
wavecode_1_r=0.200000
wavecode_1_g=0.900000
wavecode_1_b=0.800000
wavecode_1_a=1.000000
wave_1_per_point1=n=sample*6.283;
wave_1_per_point2=phs=-sample * 0.4 ;
wave_1_per_point3=tm=q1 + phs*2 - 0.01;
wave_1_per_point4=
wave_1_per_point5=flip=flip+1;
wave_1_per_point6=flip=flip*below(flip,2);
wave_1_per_point7=
wave_1_per_point8=xp=0;
wave_1_per_point9=yp=(flip*0.1-0.05)*(1-sample);
wave_1_per_point10=zp=0;
wave_1_per_point11=
wave_1_per_point12=//spin;
wave_1_per_point13=ang=-tm*23;
wave_1_per_point14=sa=sin(ang);ca=cos(ang);
wave_1_per_point15=xr=xp*sa + yp*ca;
wave_1_per_point16=yr=xp*ca - yp*sa;
wave_1_per_point17=zr=zp;
wave_1_per_point18=
wave_1_per_point19=xp=xr;
wave_1_per_point20=yp=yr + 0.05 + (sin(tm)*0.5 + 0.5)*0.2 + 0.05;
wave_1_per_point21=zp=zr;
wave_1_per_point22=
wave_1_per_point23=//wrist movement;
wave_1_per_point24=ang=sin(tm*2)*0.5 +0.5;
wave_1_per_point25=
wave_1_per_point26=xq=xp;
wave_1_per_point27=sa=sin(ang);ca=cos(ang);
wave_1_per_point28=yq=yp*sa + zp*ca;
wave_1_per_point29=zq=yp*ca - zp*sa;
wave_1_per_point30=
wave_1_per_point31=
wave_1_per_point32=ang=tm*8;
wave_1_per_point33=sa=sin(ang);ca=cos(ang);
wave_1_per_point34=xp=xq*sa + yq*ca;
wave_1_per_point35=yp=xq*ca - yq*sa;
wave_1_per_point36=zp=zq;
wave_1_per_point37=
wave_1_per_point38=//forearm movement;
wave_1_per_point39=zp=zp-0.3;
wave_1_per_point40=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_1_per_point41=xq=xp;
wave_1_per_point42=sa=sin(ang);ca=cos(ang);
wave_1_per_point43=yq=yp*sa + zp*ca;
wave_1_per_point44=zq=yp*ca - zp*sa;
wave_1_per_point45=
wave_1_per_point46=//upper arm twist
wave_1_per_point47=ang=-1.0 + cos(tm*3 + 0.5);
wave_1_per_point48=xp=xq*sa + yq*ca;
wave_1_per_point49=yp=xq*ca - yq*sa;
wave_1_per_point50=zp=zq;
wave_1_per_point51=
wave_1_per_point52=//upper arm outward;
wave_1_per_point53=zp=zp-0.35;
wave_1_per_point54=ang=cos(tm*2)*0.75 - 1.05;
wave_1_per_point55=sa=sin(ang);ca=cos(ang);
wave_1_per_point56=xq=xp*sa + zp*ca;
wave_1_per_point57=yq=yp;
wave_1_per_point58=zq=xp*ca - zp*sa;
wave_1_per_point59=
wave_1_per_point60=//upper arm up down;
wave_1_per_point61=ang=cos(tm)*0.5 - 0.5;
wave_1_per_point62=xp=xq;
wave_1_per_point63=sa=sin(ang);ca=cos(ang);
wave_1_per_point64=yp=yq*ca - zq*sa;
wave_1_per_point65=zp=yq*sa + zq*ca;
wave_1_per_point66=
wave_1_per_point67=//xp=xq;yp=yq;zp=zq;
wave_1_per_point68=
wave_1_per_point69=
wave_1_per_point70=//project into screenspace and draw on screen
wave_1_per_point71=zp=zp+2;
wave_1_per_point72=xs=xp/zp;
wave_1_per_point73=ys=yp/zp;
wave_1_per_point74=
wave_1_per_point75=x=xs+0.5;
wave_1_per_point76=y=ys*1.3+0.5;
wave_1_per_point77=
wave_1_per_point78=
wave_1_per_point79=a=(1-sample);
wave_1_per_point80=
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.000000
wavecode_2_smoothing=0.500000
wavecode_2_r=1.000000
wavecode_2_g=0.720000
wavecode_2_b=0.100000
wavecode_2_a=1.000000
wave_2_per_point1=n=sample*6.283;
wave_2_per_point2=phs=-sample * 0.4 ;
wave_2_per_point3=tm=q1 + phs*2 - 0.02;
wave_2_per_point4=
wave_2_per_point5=flip=flip+1;
wave_2_per_point6=flip=flip*below(flip,2);
wave_2_per_point7=
wave_2_per_point8=xp=0;
wave_2_per_point9=yp=(flip*0.2-0.1)*(1-sample);
wave_2_per_point10=zp=0;
wave_2_per_point11=
wave_2_per_point12=//spin;
wave_2_per_point13=ang=tm*19;
wave_2_per_point14=sa=sin(ang);ca=cos(ang);
wave_2_per_point15=xr=xp*sa + yp*ca;
wave_2_per_point16=yr=xp*ca - yp*sa;
wave_2_per_point17=zr=zp;
wave_2_per_point18=
wave_2_per_point19=xp=xr;
wave_2_per_point20=yp=yr + 0.05 + (sin(tm)*0.5 + 0.5)*0.2 + 0.05;
wave_2_per_point21=zp=zr;
wave_2_per_point22=
wave_2_per_point23=//wrist movement;
wave_2_per_point24=ang=sin(tm*2)*0.5 +0.5;
wave_2_per_point25=
wave_2_per_point26=xq=xp;
wave_2_per_point27=sa=sin(ang);ca=cos(ang);
wave_2_per_point28=yq=yp*sa + zp*ca;
wave_2_per_point29=zq=yp*ca - zp*sa;
wave_2_per_point30=
wave_2_per_point31=
wave_2_per_point32=ang=tm*8;
wave_2_per_point33=sa=sin(ang);ca=cos(ang);
wave_2_per_point34=xp=xq*sa + yq*ca;
wave_2_per_point35=yp=xq*ca - yq*sa;
wave_2_per_point36=zp=zq;
wave_2_per_point37=
wave_2_per_point38=//forearm movement;
wave_2_per_point39=zp=zp-0.3;
wave_2_per_point40=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_2_per_point41=xq=xp;
wave_2_per_point42=sa=sin(ang);ca=cos(ang);
wave_2_per_point43=yq=yp*sa + zp*ca;
wave_2_per_point44=zq=yp*ca - zp*sa;
wave_2_per_point45=
wave_2_per_point46=//upper arm twist
wave_2_per_point47=ang=-1.0 + cos(tm*3 + 0.5);
wave_2_per_point48=xp=xq*sa + yq*ca;
wave_2_per_point49=yp=xq*ca - yq*sa;
wave_2_per_point50=zp=zq;
wave_2_per_point51=
wave_2_per_point52=//upper arm outward;
wave_2_per_point53=zp=zp-0.35;
wave_2_per_point54=ang=cos(tm*2)*0.75 - 1.05;
wave_2_per_point55=sa=sin(ang);ca=cos(ang);
wave_2_per_point56=xq=xp*sa + zp*ca;
wave_2_per_point57=yq=yp;
wave_2_per_point58=zq=xp*ca - zp*sa;
wave_2_per_point59=
wave_2_per_point60=//upper arm up down;
wave_2_per_point61=ang=cos(tm)*0.5 - 0.5;
wave_2_per_point62=xp=xq;
wave_2_per_point63=sa=sin(ang);ca=cos(ang);
wave_2_per_point64=yp=yq*ca - zq*sa;
wave_2_per_point65=zp=yq*sa + zq*ca;
wave_2_per_point66=
wave_2_per_point67=//xp=xq;yp=yq;zp=zq;
wave_2_per_point68=
wave_2_per_point69=
wave_2_per_point70=//project into screenspace and draw on screen
wave_2_per_point71=zp=zp+2;
wave_2_per_point72=xs=xp/zp;
wave_2_per_point73=ys=yp/zp;
wave_2_per_point74=
wave_2_per_point75=x=xs+0.5;
wave_2_per_point76=y=ys*1.3+0.5;
wave_2_per_point77=
wave_2_per_point78=
wave_2_per_point79=a=(1-sample);
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=0
wavecode_3_scaling=1.000000
wavecode_3_smoothing=0.500000
wavecode_3_r=1.000000
wavecode_3_g=0.700000
wavecode_3_b=0.500000
wavecode_3_a=1.000000
wave_3_per_point1=n=sample*6.283;
wave_3_per_point2=phs=-sample * 0.4 ;
wave_3_per_point3=tm=q1 + phs*2 - 0.03;
wave_3_per_point4=
wave_3_per_point5=flip=flip+1;
wave_3_per_point6=flip=flip*below(flip,2);
wave_3_per_point7=
wave_3_per_point8=xp=0;
wave_3_per_point9=yp=(flip*0.3-0.15)*(1-sample);
wave_3_per_point10=zp=0;
wave_3_per_point11=
wave_3_per_point12=//spin;
wave_3_per_point13=ang=-tm*3;
wave_3_per_point14=sa=sin(ang);ca=cos(ang);
wave_3_per_point15=xr=xp*sa + yp*ca;
wave_3_per_point16=yr=xp*ca - yp*sa;
wave_3_per_point17=zr=zp;
wave_3_per_point18=
wave_3_per_point19=xp=xr;
wave_3_per_point20=yp=yr + 0.05 + (sin(tm)*0.5 + 0.5)*0.2 + 0.05;
wave_3_per_point21=zp=zr;
wave_3_per_point22=
wave_3_per_point23=//wrist movement;
wave_3_per_point24=ang=sin(tm*2)*0.5 +0.5;
wave_3_per_point25=
wave_3_per_point26=xq=xp;
wave_3_per_point27=sa=sin(ang);ca=cos(ang);
wave_3_per_point28=yq=yp*sa + zp*ca;
wave_3_per_point29=zq=yp*ca - zp*sa;
wave_3_per_point30=
wave_3_per_point31=
wave_3_per_point32=ang=tm*8;
wave_3_per_point33=sa=sin(ang);ca=cos(ang);
wave_3_per_point34=xp=xq*sa + yq*ca;
wave_3_per_point35=yp=xq*ca - yq*sa;
wave_3_per_point36=zp=zq;
wave_3_per_point37=
wave_3_per_point38=//forearm movement;
wave_3_per_point39=zp=zp-0.3;
wave_3_per_point40=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_3_per_point41=xq=xp;
wave_3_per_point42=sa=sin(ang);ca=cos(ang);
wave_3_per_point43=yq=yp*sa + zp*ca;
wave_3_per_point44=zq=yp*ca - zp*sa;
wave_3_per_point45=
wave_3_per_point46=//upper arm twist
wave_3_per_point47=ang=-1.0 + cos(tm*3 + 0.5);
wave_3_per_point48=xp=xq*sa + yq*ca;
wave_3_per_point49=yp=xq*ca - yq*sa;
wave_3_per_point50=zp=zq;
wave_3_per_point51=
wave_3_per_point52=//upper arm outward;
wave_3_per_point53=zp=zp-0.35;
wave_3_per_point54=ang=cos(tm*2)*0.75 - 1.05;
wave_3_per_point55=sa=sin(ang);ca=cos(ang);
wave_3_per_point56=xq=xp*sa + zp*ca;
wave_3_per_point57=yq=yp;
wave_3_per_point58=zq=xp*ca - zp*sa;
wave_3_per_point59=
wave_3_per_point60=//upper arm up down;
wave_3_per_point61=ang=cos(tm)*0.5 - 0.5;
wave_3_per_point62=xp=xq;
wave_3_per_point63=sa=sin(ang);ca=cos(ang);
wave_3_per_point64=yp=yq*ca - zq*sa;
wave_3_per_point65=zp=yq*sa + zq*ca;
wave_3_per_point66=
wave_3_per_point67=//xp=xq;yp=yq;zp=zq;
wave_3_per_point68=
wave_3_per_point69=
wave_3_per_point70=//project into screenspace and draw on screen
wave_3_per_point71=zp=zp+2;
wave_3_per_point72=xs=xp/zp;
wave_3_per_point73=ys=yp/zp;
wave_3_per_point74=
wave_3_per_point75=x=xs+0.5;
wave_3_per_point76=y=ys*1.3+0.5;
wave_3_per_point77=
wave_3_per_point78=
wave_3_per_point79=a=(1-sample);
shapecode_0_enabled=1
shapecode_0_sides=3
shapecode_0_additive=0
shapecode_0_thickOutline=1
shapecode_0_textured=1
shapecode_0_x=0.500000
shapecode_0_y=0.500000
shapecode_0_rad=0.375614
shapecode_0_ang=0.000000
shapecode_0_tex_ang=0.251327
shapecode_0_tex_zoom=0.498311
shapecode_0_r=1.000000
shapecode_0_g=1.000000
shapecode_0_b=1.000000
shapecode_0_a=1.000000
shapecode_0_r2=1.000000
shapecode_0_g2=1.000000
shapecode_0_b2=1.000000
shapecode_0_a2=0.000000
shapecode_0_border_r=0.000000
shapecode_0_border_g=1.000000
shapecode_0_border_b=1.000000
shapecode_0_border_a=1.000000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_x=0.500000
shapecode_1_y=0.500000
shapecode_1_rad=0.100000
shapecode_1_ang=0.000000
shapecode_1_tex_ang=0.000000
shapecode_1_tex_zoom=1.000000
shapecode_1_r=1.000000
shapecode_1_g=0.000000
shapecode_1_b=0.000000
shapecode_1_a=1.000000
shapecode_1_r2=0.000000
shapecode_1_g2=1.000000
shapecode_1_b2=0.000000
shapecode_1_a2=0.000000
shapecode_1_border_r=1.000000
shapecode_1_border_g=1.000000
shapecode_1_border_b=1.000000
shapecode_1_border_a=0.100000
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_x=0.500000
shapecode_2_y=0.500000
shapecode_2_rad=0.100000
shapecode_2_ang=0.000000
shapecode_2_tex_ang=0.000000
shapecode_2_tex_zoom=1.000000
shapecode_2_r=1.000000
shapecode_2_g=0.000000
shapecode_2_b=0.000000
shapecode_2_a=1.000000
shapecode_2_r2=0.000000
shapecode_2_g2=1.000000
shapecode_2_b2=0.000000
shapecode_2_a2=0.000000
shapecode_2_border_r=1.000000
shapecode_2_border_g=1.000000
shapecode_2_border_b=1.000000
shapecode_2_border_a=0.100000
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_x=0.500000
shapecode_3_y=0.500000
shapecode_3_rad=0.100000
shapecode_3_ang=0.000000
shapecode_3_tex_ang=0.000000
shapecode_3_tex_zoom=1.000000
shapecode_3_r=1.000000
shapecode_3_g=0.000000
shapecode_3_b=0.000000
shapecode_3_a=1.000000
shapecode_3_r2=0.000000
shapecode_3_g2=1.000000
shapecode_3_b2=0.000000
shapecode_3_a2=0.000000
shapecode_3_border_r=1.000000
shapecode_3_border_g=1.000000
shapecode_3_border_b=1.000000
shapecode_3_border_a=0.100000
per_frame_init_1=mv_x=64;mv_y=48;
per_frame_init_2=nut=0;
per_frame_init_3=stp=0;stq=0;
per_frame_init_4=rtp=0;rtq=0;
per_frame_init_5=wvr=0;
per_frame_init_6=decay=0;
per_frame_init_7=dcsp=0
per_frame_init_8=
per_frame_1=decay=0.975;
per_frame_2=
per_frame_3=vol=(bass+mid+treb)*0.25;
per_frame_4=vol=vol*vol;
per_frame_5=
per_frame_6=mtime=mtime+vol*0.01*(50/fps);
per_frame_7=
per_frame_8=q1=time*0.3;
per_frame_9=
per_frame_10=
per_frame_11=
per_frame_12=
per_pixel_1=zm=-1.015+(rad/(bass*60));
per_pixel_2=
per_pixel_3=sx=zm;
per_pixel_4=sy=zm;
