CONFIG_IDF_CMAKE=y
# 1000 Hz tick: the UAC iso IN endpoint must be serviced every 1 ms frame;
# ESP-IDF's default 100 Hz starves the audio task -> host capture fails (arecord EIO).
CONFIG_FREERTOS_HZ=1000
CONFIG_FREERTOS_WATCHPOINT_END_OF_STACK=y
CONFIG_FREERTOS_SUPPORT_STATIC_ALLOCATION=y
