/*
** ###################################################################
**     Processor:           LPC54628J512ET180
**     Compiler:            IAR ANSI C/C++ Compiler for ARM
**     Reference manual:    LPC546xx User manual Rev.1.9  5 June 2017
**     Version:             rev. 1.2, 2017-06-08
**     Build:               b241125
**
**     Abstract:
**         Linker file for the IAR ANSI C/C++ Compiler for ARM
**
**     Copyright 2016 Freescale Semiconductor, Inc.
**     Copyright 2016-2024 NXP
**     SPDX-License-Identifier: BSD-3-Clause
**
**     http:                 www.nxp.com
**     mail:                 support@nxp.com
**
** ###################################################################
*/

define symbol m_interrupts_start       = 0x00000000;
define symbol m_interrupts_end         = 0x000003FF;

define symbol m_text_start             = 0x00000400;
define symbol m_text_end               = 0x0007FFFF;

define symbol m_data_start             = 0x20000000;
define symbol m_data_end               = 0x20027FFF;

define symbol m_usb_sram_start         = 0x40100000;
define symbol m_usb_sram_end           = 0x40101FFF;

/* USB BDT size */
define symbol usb_bdt_size             = 0x0;
/* Sizes */
if (isdefinedsymbol(__stack_size__)) {
  define symbol __size_cstack__        = __stack_size__;
} else {
  define symbol __size_cstack__        = 0x0400;
}

if (isdefinedsymbol(__heap_size__)) {
  define symbol __size_heap__          = __heap_size__;
} else {
  define symbol __size_heap__          = 0x0400;
}


define memory mem with size = 4G;
define region TEXT_region = mem:[from m_interrupts_start to m_interrupts_end]
                          | mem:[from m_text_start to m_text_end];
define region DATA_region = mem:[from m_data_start to m_data_end-__size_cstack__];
define region CSTACK_region = mem:[from m_data_end-__size_cstack__+1 to m_data_end];

define block CSTACK    with alignment = 8, size = __size_cstack__   { };
define block HEAP      with alignment = 8, size = __size_heap__     { };
define block RW        { readwrite };
define block ZI        { zi };

/* regions for USB */
define region USB_BDT_region = mem:[from m_usb_sram_start to m_usb_sram_start + usb_bdt_size - 1];
define region USB_SRAM_region = mem:[from m_usb_sram_start + usb_bdt_size to m_usb_sram_end];
place in USB_BDT_region                     { section m_usb_bdt };
place in USB_SRAM_region                    { section m_usb_global };

initialize by copy { readwrite, section .textrw };

if (isdefinedsymbol(__USE_DLIB_PERTHREAD))
{
  /* Required in a multi-threaded application */
  initialize by copy with packing = none { section __DLIB_PERTHREAD };
}

do not initialize  { section .noinit, section m_usb_bdt, section m_usb_global };

place at address mem: m_interrupts_start    { readonly section .intvec };
place in TEXT_region                        { readonly };
place in DATA_region                        { block RW };
place in DATA_region                        { block ZI };
place in DATA_region                        { last block HEAP };
place in CSTACK_region                      { block CSTACK };
