<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="LPCXpresso55S69" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_19 http://mcuxpresso.nxp.com/XSD/mex_configuration_19.xsd" uuid="acf73d26-2bf9-4855-b3be-26068672d98a" version="19" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_19" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>LPC55S69</processor>
      <package>LPC55S69JBD100</package>
      <board>LPCXpresso55S69</board>
      <board_revision>A2</board_revision>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="cm33_core0">
         <core name="Cortex-M33 (Core #0)" id="cm33_core0" description=""/>
         <core name="Cortex-M33 (Core #1)" id="cm33_core1" description=""/>
      </cores>
      <description></description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <custom_copyright>
         <text>/*
 * Copyright 2026 NXP
 * All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */
</text>
         <enabled>true</enabled>
      </custom_copyright>
      <update_include_paths>true</update_include_paths>
      <enable_parallel_routing>true</enable_parallel_routing>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="17.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>25.09.10</processor_version>
            <pin_labels>
               <pin_label pin_num="7" pin_signal="PIO0_1/FC3_CTS_SDA_SSEL0/CT_INP0/SCT_GPI1/SD1_CLK/CMP0_OUT/SECURE_GPIO0_1" label="P18[2]/SD1_CLK" identifier="LED_RED"/>
               <pin_label pin_num="88" pin_signal="PIO0_5/FC4_RXD_SDA_MOSI_DATA/CTIMER3_MAT0/SCT_GPI5/FC3_RTS_SCL_SSEL1/MCLK/SECURE_GPIO0_5" label="S1/J10[1]/U3[12]/P17[8]/P7[7]/U11[4]/P0_5-ISP1" identifier="LED"/>
               <pin_label pin_num="11" pin_signal="PIO1_0/FC0_RTS_SCL_SSEL1/SD0_D3/CT_INP2/SCT_GPI4/PLU_OUT3/ADC0_11" label="U20[2]/SD0_D3" identifier="BUTTON"/>
            </pin_labels>
            <expansion_headers>
               <expansion_header id="lpc_style_arduino" name="LPCXpresso V3 (Arduino compatible)">
                  <connectors>
                     <connector id="C1" name="P16">
                        <pins>
                           <pin id="8" external_signal_types="power_supply_3.3V" name="3.3V"/>
                           <pin id="10" pin_num="32" pin_signal="RESETN" name="RESET"/>
                           <pin id="12" external_signal_types="power_supply_3.3V" name="3.3V"/>
                           <pin id="14" external_signal_types="power_supply_5V" name="5V"/>
                           <pin id="16" external_signal_types="ground" name="GND"/>
                           <pin id="18" external_signal_types="ground" name="GND"/>
                           <pin id="20" external_signal_types="power_supply_5V" name="5V"/>
                        </pins>
                     </connector>
                     <connector id="C2" name="P17">
                        <pins>
                           <pin id="1" pin_num="4" pin_signal="PIO1_20/FC7_RTS_SCL_SSEL1/CT_INP14/FC4_TXD_SCL_MISO_WS/PLU_OUT2" name="D15"/>
                           <pin id="3" pin_num="30" pin_signal="PIO1_21/FC7_CTS_SDA_SSEL0/CTIMER3_MAT2/FC4_RXD_SDA_MOSI_DATA/PLU_OUT3" name="D14"/>
                           <pin id="5" external_signal_types="power_supply_3.3V" name="3.3V"/>
                           <pin id="6" pin_num="93" pin_signal="PIO1_11/FC1_TXD_SCL_MISO_WS/CT_INP5/USB0_VBUS"/>
                           <pin id="7" external_signal_types="ground" name="GND"/>
                           <pin id="8" pin_num="88" pin_signal="PIO0_5/FC4_RXD_SDA_MOSI_DATA/CTIMER3_MAT0/SCT_GPI5/FC3_RTS_SCL_SSEL1/MCLK/SECURE_GPIO0_5"/>
                           <pin id="9" pin_num="61" pin_signal="PIO1_2/CTIMER0_MAT3/SCT_GPI6/HS_SPI_SCK/USB1_PORTPWRN/PLU_OUT5" name="D13"/>
                           <pin id="10" pin_num="74" pin_signal="PIO0_20/FC3_CTS_SDA_SSEL0/CTIMER1_MAT1/CT_INP15/SCT_GPI2/FC7_RXD_SDA_MOSI_DATA/HS_SPI_SSEL0/PLU_IN5/SECURE_GPIO0_20/FC4_TXD_SCL_MISO_WS"/>
                           <pin id="11" pin_num="62" pin_signal="PIO1_3/SCT0_OUT4/HS_SPI_MISO/USB0_PORTPWRN/PLU_OUT6" name="D12"/>
                           <pin id="12" pin_num="90" pin_signal="PIO0_19/FC4_RTS_SCL_SSEL1/UTICK_CAP0/CTIMER0_MAT2/SCT0_OUT2/FC7_TXD_SCL_MISO_WS/PLU_IN4/SECURE_GPIO0_19"/>
                           <pin id="13" pin_num="60" pin_signal="PIO0_26/FC2_RXD_SDA_MOSI_DATA/CLKOUT/CT_INP14/SCT0_OUT5/USB0_IDVALUE/FC0_SCK/HS_SPI_MOSI/SECURE_GPIO0_26" name="D11"/>
                           <pin id="14" pin_num="76" pin_signal="PIO0_21/FC3_RTS_SCL_SSEL1/UTICK_CAP3/CTIMER3_MAT3/SCT_GPI3/FC7_SCK/PLU_CLKIN/SECURE_GPIO0_21"/>
                           <pin id="15" pin_num="59" pin_signal="PIO1_1/FC3_RXD_SDA_MOSI_DATA/CT_INP3/SCT_GPI5/HS_SPI_SSEL1/USB1_OVERCURRENTN/PLU_OUT4" name="D10"/>
                           <pin id="16" pin_num="85" pin_signal="PIO1_27/FC2_RTS_SCL_SSEL1/SD0_D4/CTIMER0_MAT3/CLKOUT/PLU_IN4"/>
                           <pin id="17" pin_num="31" pin_signal="PIO1_5/FC0_RXD_SDA_MOSI_DATA/SD0_D2/CTIMER2_MAT0/SCT_GPI0" name="D9"/>
                           <pin id="18" pin_num="73" pin_signal="PIO1_28/FC7_SCK/SD0_D5/CT_INP2/PLU_IN3"/>
                           <pin id="19" pin_num="24" pin_signal="PIO1_8/FC0_CTS_SDA_SSEL0/SD0_CLK/SCT0_OUT1/FC4_SSEL2/ADC0_4" name="D8"/>
                           <pin id="20" pin_num="2" pin_signal="PIO1_13/FC6_RXD_SDA_MOSI_DATA/CT_INP6/USB0_OVERCURRENTN/USB0_FRAME/SD0_CARD_DET_N"/>
                        </pins>
                     </connector>
                     <connector id="C3" name="P18">
                        <pins>
                           <pin id="1" pin_num="10" pin_signal="PIO1_9/FC1_SCK/CT_INP4/SCT0_OUT2/FC4_CTS_SDA_SSEL0/ADC0_12" name="D7"/>
                           <pin id="2" pin_num="7" pin_signal="PIO0_1/FC3_CTS_SDA_SSEL0/CT_INP0/SCT_GPI1/SD1_CLK/CMP0_OUT/SECURE_GPIO0_1"/>
                           <pin id="3" pin_num="40" pin_signal="PIO1_10/FC1_RXD_SDA_MOSI_DATA/CTIMER1_MAT0/SCT0_OUT3" name="D6"/>
                           <pin id="4" pin_num="57" pin_signal="PIO1_14/UTICK_CAP2/CTIMER1_MAT2/FC5_CTS_SDA_SSEL0/USB0_LEDN/SD1_CMD/ACMP0_D"/>
                           <pin id="5" pin_num="1" pin_signal="PIO1_4/FC0_SCK/SD0_D0/CTIMER2_MAT1/SCT0_OUT0/FREQME_GPIO_CLK_A" name="D5"/>
                           <pin id="6" pin_num="77" pin_signal="PIO1_25/FC2_TXD_SCL_MISO_WS/SCT0_OUT2/SD1_D0/UTICK_CAP0/PLU_CLKIN"/>
                           <pin id="7" pin_num="9" pin_signal="PIO1_7/FC0_RTS_SCL_SSEL1/SD0_D1/CTIMER2_MAT2/SCT_GPI4" name="D4-LED_GREEN"/>
                           <pin id="8" pin_num="42" pin_signal="PIO1_23/FC2_SCK/SCT0_OUT0/SD1_D3/FC3_SSEL2/PLU_OUT5"/>
                           <pin id="10" pin_num="3" pin_signal="PIO1_24/FC2_RXD_SDA_MOSI_DATA/SCT0_OUT1/SD1_D1/FC3_SSEL3/PLU_OUT6"/>
                           <pin id="11" pin_num="22" pin_signal="PIO0_15/FC6_CTS_SDA_SSEL0/UTICK_CAP2/CT_INP16/SCT0_OUT2/SD0_WR_PRT/SECURE_GPIO0_15/ADC0_2" name="D2"/>
                           <pin id="12" pin_num="82" pin_signal="PIO1_15/UTICK_CAP3/CT_INP7/FC5_RTS_SCL_SSEL1/FC4_RTS_SCL_SSEL1/SD1_D2"/>
                           <pin id="13" pin_num="27" pin_signal="PIO0_27/FC2_TXD_SCL_MISO_WS/CTIMER3_MAT2/SCT0_OUT6/FC7_RXD_SDA_MOSI_DATA/PLU_OUT0/SECURE_GPIO0_27" name="D1"/>
                           <pin id="14" pin_num="58" pin_signal="PIO1_19/SCT0_OUT7/CTIMER3_MAT1/SCT_GPI7/FC4_SCK/PLU_OUT1/ACMPVREF"/>
                           <pin id="15" pin_num="3" pin_signal="PIO1_24/FC2_RXD_SDA_MOSI_DATA/SCT0_OUT1/SD1_D1/FC3_SSEL3/PLU_OUT6" name="D0"/>
                           <pin id="16" pin_num="64" pin_signal="PIO1_18/SD1_POW_EN/SCT0_OUT5/PLU_OUT0"/>
                           <pin id="17" pin_num="87" pin_signal="PIO1_16/FC6_TXD_SCL_MISO_WS/CTIMER1_MAT3/SD0_CMD"/>
                           <pin id="18" pin_num="68" pin_signal="PIO1_26/FC2_CTS_SDA_SSEL0/SCT0_OUT3/CT_INP3/UTICK_CAP1/HS_SPI_SSEL3/PLU_IN5"/>
                           <pin id="19" pin_num="43" pin_signal="PIO1_17/FC6_RTS_SCL_SSEL1/SCT0_OUT4/SD1_CARD_INT_N/SD1_CARD_DET_N"/>
                           <pin id="20" pin_num="56" pin_signal="PIO0_18/FC4_CTS_SDA_SSEL0/SD0_WR_PRT/CTIMER1_MAT0/SCT0_OUT1/PLU_IN3/SECURE_GPIO0_18/ACMP0_C"/>
                        </pins>
                     </connector>
                     <connector id="C4" name="P19">
                        <pins>
                           <pin id="2" pin_num="14" pin_signal="PIO0_16/FC4_TXD_SCL_MISO_WS/CLKOUT/CT_INP4/SECURE_GPIO0_16/ADC0_8" name="A0"/>
                           <pin id="4" pin_num="20" pin_signal="PIO0_23/MCLK/CTIMER1_MAT2/CTIMER3_MAT3/SCT0_OUT4/FC0_CTS_SDA_SSEL0/SD1_D1/SECURE_GPIO0_23/ADC0_0" name="A1"/>
                           <pin id="6" pin_num="54" pin_signal="PIO0_0/FC3_SCK/CTIMER0_MAT0/SCT_GPI0/SD1_CARD_INT_N/SECURE_GPIO0_0/ACMP0_A" name="A2"/>
                           <pin id="7" pin_num="91" pin_signal="PIO1_31/MCLK/SD1_CLK/CTIMER0_MAT2/SCT0_OUT6/PLU_IN0"/>
                           <pin id="8" pin_num="91" pin_signal="PIO1_31/MCLK/SD1_CLK/CTIMER0_MAT2/SCT0_OUT6/PLU_IN0" name="A3"/>
                           <pin id="9" pin_num="71" pin_signal="PIO0_13/FC1_CTS_SDA_SSEL0/UTICK_CAP0/CT_INP0/SCT_GPI0/FC1_RXD_SDA_MOSI_DATA/PLU_IN0/SECURE_GPIO0_13"/>
                           <pin id="10" pin_num="71" pin_signal="PIO0_13/FC1_CTS_SDA_SSEL0/UTICK_CAP0/CT_INP0/SCT_GPI0/FC1_RXD_SDA_MOSI_DATA/PLU_IN0/SECURE_GPIO0_13" name="A4"/>
                           <pin id="11" pin_num="72" pin_signal="PIO0_14/FC1_RTS_SCL_SSEL1/UTICK_CAP1/CT_INP1/SCT_GPI1/FC1_TXD_SCL_MISO_WS/PLU_IN1/SECURE_GPIO0_14"/>
                           <pin id="12" pin_num="72" pin_signal="PIO0_14/FC1_RTS_SCL_SSEL1/UTICK_CAP1/CT_INP1/SCT_GPI1/FC1_TXD_SCL_MISO_WS/PLU_IN1/SECURE_GPIO0_14" name="A5"/>
                        </pins>
                     </connector>
                  </connectors>
               </expansion_header>
            </expansion_headers>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitDEBUG_UARTPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="FLEXCOMM0" description="Peripheral FLEXCOMM0 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_iocon" description="Pins initialization requires the LPC_IOCON Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="FLEXCOMM0" signal="RXD_SDA_MOSI_DATA" pin_num="92" pin_signal="PIO0_29/FC0_RXD_SDA_MOSI_DATA/SD1_D2/CTIMER2_MAT3/SCT0_OUT8/CMP0_OUT/PLU_OUT2/SECURE_GPIO0_29">
                     <pin_features>
                        <pin_feature name="mode" value="inactive"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM0" signal="TXD_SCL_MISO_WS" pin_num="94" pin_signal="PIO0_30/FC0_TXD_SCL_MISO_WS/SD1_D3/CTIMER0_MAT0/SCT0_OUT9/SECURE_GPIO0_30">
                     <pin_features>
                        <pin_feature name="mode" value="inactive"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitSWD_DEBUGPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SWD" description="Peripheral SWD signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitSWD_DEBUGPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitSWD_DEBUGPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_iocon" description="Pins initialization requires the LPC_IOCON Driver in the project." problem_level="2" source="Pins:BOARD_InitSWD_DEBUGPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="SWD" signal="SWCLK" pin_num="13" pin_signal="PIO0_11/FC6_RXD_SDA_MOSI_DATA/CTIMER2_MAT2/FREQME_GPIO_CLK_A/SWCLK/SECURE_GPIO0_11/ADC0_9">
                     <pin_features>
                        <pin_feature name="mode" value="pullDown"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                        <pin_feature name="asw" value="enabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="SWD" signal="SWDIO" pin_num="12" pin_signal="PIO0_12/FC3_TXD_SCL_MISO_WS/SD1_BACKEND_PWR/FREQME_GPIO_CLK_B/SCT_GPI7/SD0_POW_EN/SWDIO/FC6_TXD_SCL_MISO_WS/SECURE_GPIO0_12/ADC0_10">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                        <pin_feature name="asw" value="enabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="SWD" signal="SWO" pin_num="21" pin_signal="PIO0_10/FC6_SCK/CT_INP10/CTIMER2_MAT0/FC1_TXD_SCL_MISO_WS/SCT0_OUT2/SWO/SECURE_GPIO0_10/ADC0_1">
                     <pin_features>
                        <pin_feature name="identifier" value="DEBUG_SWD_SWO"/>
                        <pin_feature name="mode" value="inactive"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                        <pin_feature name="asw" value="disabled"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitUSBPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="USBFSH" description="Peripheral USBFSH signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitUSBPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="USBHSH" description="Peripheral USBHSH signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitUSBPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitUSBPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_iocon" description="Pins initialization requires the LPC_IOCON Driver in the project." problem_level="2" source="Pins:BOARD_InitUSBPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="USBFSH" signal="USB_DP" pin_num="97" pin_signal="USB0_DP"/>
                  <pin peripheral="USBFSH" signal="USB_DM" pin_num="98" pin_signal="USB0_DM"/>
                  <pin peripheral="USBFSH" signal="USB_VBUS" pin_num="78" pin_signal="PIO0_22/FC6_TXD_SCL_MISO_WS/UTICK_CAP1/CT_INP15/SCT0_OUT3/USB0_VBUS/SD1_D0/PLU_OUT7/SECURE_GPIO0_22">
                     <pin_features>
                        <pin_feature name="mode" value="inactive"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="USBHSH" signal="USB_DM" pin_num="35" pin_signal="USB1_DM"/>
                  <pin peripheral="USBHSH" signal="USB_DP" pin_num="34" pin_signal="USB1_DP"/>
                  <pin peripheral="USBHSH" signal="USB_VBUS" pin_num="36" pin_signal="USB1_VBUS"/>
                  <pin peripheral="USBHSH" signal="USB_OVERCURRENTN" pin_num="65" pin_signal="PIO1_30/FC7_TXD_SCL_MISO_WS/SD0_D7/SCT_GPI7/USB1_OVERCURRENTN/USB1_LEDN/PLU_IN1">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="USBFSH" signal="USB_OVERCURRENTN" pin_num="66" pin_signal="PIO0_28/FC0_SCK/SD1_CMD/CT_INP11/SCT0_OUT7/USB0_OVERCURRENTN/PLU_OUT1/SECURE_GPIO0_28">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="USBFSH" signal="USB_PORTPWRN" pin_num="67" pin_signal="PIO1_12/FC6_SCK/CTIMER1_MAT1/USB0_PORTPWRN/HS_SPI_SSEL2">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="USBHSH" signal="USB_PORTPWRN" pin_num="80" pin_signal="PIO1_29/FC7_RXD_SDA_MOSI_DATA/SD0_D6/SCT_GPI6/USB1_PORTPWRN/USB1_FRAME/PLU_IN2">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitLEDsPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitLEDsPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_gpio" description="Pins initialization requires the LPC_GPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitLEDsPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIO" signal="PIO0, 5" pin_num="88" pin_signal="PIO0_5/FC4_RXD_SDA_MOSI_DATA/CTIMER3_MAT0/SCT_GPI5/FC3_RTS_SCL_SSEL1/MCLK/SECURE_GPIO0_5">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="gpio_init_state" value="true"/>
                        <pin_feature name="mode" value="pullUp"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitBUTTONsPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SYSCON" description="Peripheral SYSCON signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitBUTTONsPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitBUTTONsPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_gpio" description="Pins initialization requires the LPC_GPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitBUTTONsPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="SYSCON" signal="RESET" pin_num="32" pin_signal="RESETN"/>
                  <pin peripheral="GPIO" signal="PIO1, 0" pin_num="11" pin_signal="PIO1_0/FC0_RTS_SCL_SSEL1/SD0_D3/CT_INP2/SCT_GPI4/PLU_OUT3/ADC0_11">
                     <pin_features>
                        <pin_feature name="direction" value="INPUT"/>
                        <pin_feature name="mode" value="pullUp"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitPins_Core0">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins_Core0">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins/>
            </function>
            <function name="BOARD_InitPins_Core1">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm33_core1</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins_Core1">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins/>
            </function>
            <function name="BOARD_InitI2SPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="FLEXCOMM4" description="Peripheral FLEXCOMM4 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitI2SPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="SYSCON" description="Peripheral SYSCON signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitI2SPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="FLEXCOMM7" description="Peripheral FLEXCOMM7 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitI2SPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="Peripheral" resourceId="FLEXCOMM6" description="Peripheral FLEXCOMM6 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitI2SPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitI2SPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_iocon" description="Pins initialization requires the LPC_IOCON Driver in the project." problem_level="2" source="Pins:BOARD_InitI2SPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="FLEXCOMM4" signal="TXD_SCL_MISO_WS" pin_num="4" pin_signal="PIO1_20/FC7_RTS_SCL_SSEL1/CT_INP14/FC4_TXD_SCL_MISO_WS/PLU_OUT2">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM4" signal="RXD_SDA_MOSI_DATA" pin_num="30" pin_signal="PIO1_21/FC7_CTS_SDA_SSEL0/CTIMER3_MAT2/FC4_RXD_SDA_MOSI_DATA/PLU_OUT3">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="SYSCON" signal="MCLK" pin_num="91" pin_signal="PIO1_31/MCLK/SD1_CLK/CTIMER0_MAT2/SCT0_OUT6/PLU_IN0">
                     <pin_features>
                        <pin_feature name="mode" value="inactive"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM7" signal="SCK" pin_num="76" pin_signal="PIO0_21/FC3_RTS_SCL_SSEL1/UTICK_CAP3/CTIMER3_MAT3/SCT_GPI3/FC7_SCK/PLU_CLKIN/SECURE_GPIO0_21">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM7" signal="RXD_SDA_MOSI_DATA" pin_num="74" pin_signal="PIO0_20/FC3_CTS_SDA_SSEL0/CTIMER1_MAT1/CT_INP15/SCT_GPI2/FC7_RXD_SDA_MOSI_DATA/HS_SPI_SSEL0/PLU_IN5/SECURE_GPIO0_20/FC4_TXD_SCL_MISO_WS">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM7" signal="TXD_SCL_MISO_WS" pin_num="90" pin_signal="PIO0_19/FC4_RTS_SCL_SSEL1/UTICK_CAP0/CTIMER0_MAT2/SCT0_OUT2/FC7_TXD_SCL_MISO_WS/PLU_IN4/SECURE_GPIO0_19">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM6" signal="SCK" pin_num="21" pin_signal="PIO0_10/FC6_SCK/CT_INP10/CTIMER2_MAT0/FC1_TXD_SCL_MISO_WS/SCT0_OUT2/SWO/SECURE_GPIO0_10/ADC0_1">
                     <pin_features>
                        <pin_feature name="identifier" value="FC6_I2S_CLK"/>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                        <pin_feature name="asw" value="enabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM6" signal="RXD_SDA_MOSI_DATA" pin_num="2" pin_signal="PIO1_13/FC6_RXD_SDA_MOSI_DATA/CT_INP6/USB0_OVERCURRENTN/USB0_FRAME/SD0_CARD_DET_N">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM6" signal="TXD_SCL_MISO_WS" pin_num="87" pin_signal="PIO1_16/FC6_TXD_SCL_MISO_WS/CTIMER1_MAT3/SD0_CMD">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitACCELPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>false</callFromInitBoot>
                  <coreID>cm33_core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="FLEXCOMM4" description="Peripheral FLEXCOMM4 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitACCELPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitACCELPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_gpio" description="Pins initialization requires the LPC_GPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitACCELPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.lpc_iocon" description="Pins initialization requires the LPC_IOCON Driver in the project." problem_level="2" source="Pins:BOARD_InitACCELPins">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="FLEXCOMM4" signal="RXD_SDA_MOSI_DATA" pin_num="30" pin_signal="PIO1_21/FC7_CTS_SDA_SSEL0/CTIMER3_MAT2/FC4_RXD_SDA_MOSI_DATA/PLU_OUT3">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="FLEXCOMM4" signal="TXD_SCL_MISO_WS" pin_num="4" pin_signal="PIO1_20/FC7_RTS_SCL_SSEL1/CT_INP14/FC4_TXD_SCL_MISO_WS/PLU_OUT2">
                     <pin_features>
                        <pin_feature name="mode" value="pullUp"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO" signal="PIO1, 19" pin_num="58" pin_signal="PIO1_19/SCT0_OUT7/CTIMER3_MAT1/SCT_GPI7/FC4_SCK/PLU_OUT1/ACMPVREF">
                     <pin_features>
                        <pin_feature name="direction" value="INPUT"/>
                        <pin_feature name="mode" value="inactive"/>
                        <pin_feature name="slew_rate" value="standard"/>
                        <pin_feature name="invert" value="disabled"/>
                        <pin_feature name="open_drain" value="disabled"/>
                        <pin_feature name="asw" value="disabled"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="18.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>25.09.10</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockFRO12M" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO12M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO12M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO12M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO12M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO12M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFRO12M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="System_clock.outFreq" value="12 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings/>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockFROHF96M" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFROHF96M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFROHF96M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFROHF96M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFROHF96M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFROHF96M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockFROHF96M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="ANACTRL.fro_hf.outFreq" value="96 MHz" locked="false" enabled="false"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="System_clock.outFreq" value="96 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="ANALOG_CONTROL_FRO192M_CTRL_ENDI_FRO_96M_CFG" value="Enable" locked="false"/>
                  <setting id="SYSCON.MAINCLKSELA.sel" value="ANACTRL.fro_hf_clk" locked="false"/>
               </clock_settings>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockPLL100M" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALIN" description="&apos;XTALIN&apos; (Pins tool id: SYSCON.XTALIN, Clocks tool id: SYSCON.XTALIN) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALIN" description="&apos;XTALIN&apos; (Pins tool id: SYSCON.XTALIN, Clocks tool id: SYSCON.XTALIN) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALOUT" description="&apos;XTALOUT&apos; (Pins tool id: SYSCON.XTALOUT, Clocks tool id: SYSCON.XTALOUT) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALOUT" description="&apos;XTALOUT&apos; (Pins tool id: SYSCON.XTALOUT, Clocks tool id: SYSCON.XTALOUT) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL100M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="SYSCON.XTAL32M.outFreq" value="16 MHz" locked="false" enabled="true"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="System_clock.outFreq" value="100 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="PLL0_Mode" value="Normal" locked="false"/>
                  <setting id="ENABLE_CLKIN_ENA" value="Enabled" locked="false"/>
                  <setting id="ENABLE_SYSTEM_CLK_OUT" value="Enabled" locked="false"/>
                  <setting id="SYSCON.MAINCLKSELB.sel" value="SYSCON.PLL0_BYPASS" locked="false"/>
                  <setting id="SYSCON.PLL0CLKSEL.sel" value="SYSCON.CLK_IN_EN" locked="false"/>
                  <setting id="SYSCON.PLL0M_MULT.scale" value="100" locked="true"/>
                  <setting id="SYSCON.PLL0N_DIV.scale" value="4" locked="true"/>
                  <setting id="SYSCON.PLL0_PDEC.scale" value="4" locked="true"/>
               </clock_settings>
               <called_from_default_init>false</called_from_default_init>
            </clock_configuration>
            <clock_configuration name="BOARD_BootClockPLL150M" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALIN" description="&apos;XTALIN&apos; (Pins tool id: SYSCON.XTALIN, Clocks tool id: SYSCON.XTALIN) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALIN" description="&apos;XTALIN&apos; (Pins tool id: SYSCON.XTALIN, Clocks tool id: SYSCON.XTALIN) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALOUT" description="&apos;XTALOUT&apos; (Pins tool id: SYSCON.XTALOUT, Clocks tool id: SYSCON.XTALOUT) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="SYSCON.XTALOUT" description="&apos;XTALOUT&apos; (Pins tool id: SYSCON.XTALOUT, Clocks tool id: SYSCON.XTALOUT) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.power" description="Clocks initialization requires the POWER Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core1">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockPLL150M">
                     <feature name="enabled" evaluation="equal" configuration="cm33_core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="SYSCON.XTAL32M.outFreq" value="16 MHz" locked="false" enabled="true"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="FXCOM0_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="144 MHz" locked="false" accuracy=""/>
                  <clock_output id="USB0_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="USB1_PHY_clock.outFreq" value="16 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="PLL0_Mode" value="Normal" locked="false"/>
                  <setting id="PLL1_Mode" value="Normal" locked="false"/>
                  <setting id="ENABLE_CLKIN_ENA" value="Enabled" locked="false"/>
                  <setting id="ENABLE_PLL_USB_OUT" value="Enabled" locked="false"/>
                  <setting id="ENABLE_SYSTEM_CLK_OUT" value="Enabled" locked="false"/>
                  <setting id="SYSCON.FCCLKSEL0.sel" value="SYSCON.PLL0DIV" locked="false"/>
                  <setting id="SYSCON.FRGCTRL0_DIV.scale" value="400" locked="false"/>
                  <setting id="SYSCON.MAINCLKSELB.sel" value="SYSCON.PLL1_BYPASS" locked="false"/>
                  <setting id="SYSCON.PLL0CLKSEL.sel" value="SYSCON.CLK_IN_EN" locked="false"/>
                  <setting id="SYSCON.PLL0DIV.scale" value="2" locked="false"/>
                  <setting id="SYSCON.PLL0M_MULT.scale" value="150" locked="true"/>
                  <setting id="SYSCON.PLL0N_DIV.scale" value="8" locked="true"/>
                  <setting id="SYSCON.PLL0_PDEC.scale" value="2" locked="true"/>
                  <setting id="SYSCON.PLL1CLKSEL.sel" value="SYSCON.CLK_IN_EN" locked="false"/>
                  <setting id="SYSCON.PLL1M_MULT.scale" value="18" locked="false"/>
                  <setting id="SYSCON.PLL1_PDEC.scale" value="2" locked="false"/>
                  <setting id="SYSCON.USB0CLKDIV.scale" value="3" locked="false"/>
                  <setting id="SYSCON.USB0CLKSEL.sel" value="SYSCON.MAINCLKSELB" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="2.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <dcdx_profile>
            <processor_version>0.0.0</processor_version>
         </dcdx_profile>
         <dcdx_configurations/>
      </dcdx>
      <periphs name="Peripherals" version="15.0" enabled="true" update_project_code="true">
         <dependencies>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.flexcomm_usart" description="FLEXCOMM USART Driver is not found in the toolchain/IDE project. The project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.flexcomm_usart" description="An unsupported version of the FLEXCOMM USART Driver in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. The project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">2.2.0</data>
               </feature>
            </dependency>
            <dependency resourceType="Tool" resourceId="Clocks" description="The Clocks tool is required by the Peripherals tool, but it is disabled." problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data>true</data>
               </feature>
            </dependency>
         </dependencies>
         <generated_project_files>
            <file path="board/peripherals.c" update_enabled="true"/>
            <file path="board/peripherals.h" update_enabled="true"/>
         </generated_project_files>
         <peripherals_profile>
            <processor_version>25.09.10</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals_cm33_core0" uuid="61d0725d-b300-49cb-9c66-b5edfbf8ffc1" called_from_default_init="true" id_prefix="" core="cm33_core0">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="ClockOutput" resourceId="FXCOM0_clock" description="FXCOM0 clock is inactive." problem_level="2" source="Peripherals:BOARD_InitPeripherals_cm33_core0">
                     <feature name="frequency" evaluation="greaterThan">
                        <data type="Frequency" unit="Hz">0</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="FLEXCOMM0.usart_rxd" description="Signal RX is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals_cm33_core0">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="FLEXCOMM0.usart_txd" description="Signal TX is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals_cm33_core0">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <instances>
                  <instance name="ACCEL" uuid="b999c56a-0d01-4089-9311-9224db5272f4" type="flexcomm_i2c" type_id="flexcomm_i2c_2.3.0" mode="I2C_Polling" peripheral="FLEXCOMM4" enabled="false" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="fsl_i2c" quick_selection="QS_I2C_Master">
                        <setting name="i2c_mode" value="kI2C_Master"/>
                        <setting name="clockSource" value="FXCOMFunctionClock"/>
                        <setting name="clockSourceFreq" value="ClocksTool_DefaultInit"/>
                        <struct name="i2c_master_config">
                           <setting name="enableMaster" value="true"/>
                           <setting name="baudRate_Bps" value="100000"/>
                           <setting name="enableTimeout" value="false"/>
                           <setting name="timeout_Ms" value="35"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="DEBUG_UART" uuid="9fb0504c-6159-43e2-98bb-51d75f06133a" type="flexcomm_usart" type_id="flexcomm_usart_2.2.0" mode="polling" peripheral="FLEXCOMM0" enabled="true" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="usartConfig_t">
                        <struct name="usartConfig">
                           <setting name="clockSource" value="FXCOMFunctionClock"/>
                           <setting name="clockSourceFreq" value="ClocksTool_DefaultInit"/>
                           <setting name="baudRate_Bps" value="115200"/>
                           <setting name="syncMode" value="kUSART_SyncModeDisabled"/>
                           <setting name="parityMode" value="kUSART_ParityDisabled"/>
                           <setting name="stopBitCount" value="kUSART_OneStopBit"/>
                           <setting name="bitCountPerChar" value="kUSART_8BitsPerChar"/>
                           <setting name="loopback" value="false"/>
                           <setting name="txWatermark" value="kUSART_TxFifo0"/>
                           <setting name="rxWatermark" value="kUSART_RxFifo1"/>
                           <setting name="enableRx" value="true"/>
                           <setting name="enableTx" value="true"/>
                           <setting name="clockPolarity" value="kUSART_RxSampleOnFallingEdge"/>
                           <setting name="enableContinuousSCLK" value="false"/>
                        </struct>
                     </config_set>
                  </instance>
                  <instance name="LEDS" uuid="f5ad3a56-404b-44cb-8abc-7b25b5551d33" type="lpc_gpio" type_id="lpc_gpio_2.1.1" mode="GPIO" peripheral="GPIO" enabled="false" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="lpc_gpio"/>
                  </instance>
                  <instance name="SW" uuid="d57ddfca-dc72-486c-a145-c7a2ab1e1a66" type="lpc_gpio" type_id="lpc_gpio_2.1.1" mode="GPIO" peripheral="GPIO" enabled="false" comment="" custom_name_enabled="true" editing_lock="false">
                     <config_set name="lpc_gpio"/>
                  </instance>
                  <instance name="NVIC" uuid="56761ad9-9b77-4074-917d-de0fde10cd48" type="nvic" type_id="nvic" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
            <functional_group name="BOARD_InitPeripherals_cm33_core1" uuid="e2041cd4-ebb6-45a5-807f-e0c2dc047d48" called_from_default_init="false" id_prefix="" core="cm33_core1">
               <description></description>
               <options/>
               <dependencies/>
               <instances>
                  <instance name="NVIC_2" uuid="db546092-4c45-40af-938a-8cc58edd1c4f" type="nvic" type_id="nvic" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="905d2747-654a-47d9-91f9-81a5c6f9c407" type_id="system">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
                  <setting name="global_init" value=""/>
               </config_set_global>
            </component>
            <component name="msg" uuid="64cbcd7c-424d-4baf-9681-a60878969fb6" type_id="msg">
               <config_set_global name="global_messages"/>
            </component>
            <component name="generic_can" uuid="b9b018dd-ef4e-41f6-b456-f91b855cb391" type_id="generic_can">
               <config_set_global name="global_can"/>
            </component>
            <component name="uart_cmsis_common" uuid="bafa6375-9184-4272-8102-06ea086041d7" type_id="uart_cmsis_common">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="generic_uart" uuid="1710dc7f-381f-4b37-8f78-0fd2f923b3ac" type_id="generic_uart">
               <config_set_global name="global_uart"/>
            </component>
            <component name="generic_enet" uuid="c7fc4395-b141-4b13-a326-4145e765b2b7" type_id="generic_enet">
               <config_set_global name="global_enet"/>
            </component>
            <component name="gpio_adapter_common" uuid="b6ee89c2-4c58-4181-94dc-af13d8ae8ea5" type_id="gpio_adapter_common">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="10.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>0.0.0</processor_version>
            <tool_options>
               <option id="_output_type_" value="c_code"/>
               <option id="_legacy_source_names_" value="yes"/>
            </tool_options>
         </tee_profile>
         <functional_group name="BOARD_InitTrustZone" called_from_default_init="true" id_prefix="" prefix_user_defined="true">
            <description></description>
            <options/>
            <ahb>
               <relative_region start="0" size="655360" security="s_priv" memory="PROGRAM_FLASH"/>
               <relative_region start="0" size="131072" security="s_priv" memory="BootROM"/>
               <relative_region start="0" size="32768" security="s_priv" memory="SRAMX"/>
               <relative_region start="0" size="65536" security="s_priv" memory="SRAM0"/>
               <relative_region start="0" size="65536" security="s_priv" memory="SRAM1"/>
               <relative_region start="0" size="65536" security="s_priv" memory="SRAM2"/>
               <relative_region start="0" size="65536" security="s_priv" memory="SRAM3"/>
               <relative_region start="0" size="16384" security="s_priv" memory="SRAM4"/>
               <relative_region start="0" size="16384" security="s_priv" memory="AHBperipherals_port10_ahb_secure_ctrl_area"/>
               <relative_region start="0" size="16384" security="s_priv" memory="USB_RAM"/>
               <masters>
                  <master id="HASH" security="ns_user"/>
                  <master id="MCM33C" security="ns_user"/>
                  <master id="MCM33S" security="ns_user"/>
                  <master id="PQ" security="ns_user"/>
                  <master id="SDIO" security="ns_user"/>
                  <master id="SDMA0" security="ns_user"/>
                  <master id="SDMA1" security="ns_user"/>
                  <master id="USBFSD" security="ns_user"/>
                  <master id="USBFSH" security="ns_user"/>
               </masters>
               <peripherals>
                  <peripheral id="ADC0" security="s_priv"/>
                  <peripheral id="AHB_SECURE_CTRL" security="s_priv"/>
                  <peripheral id="ANACTRL" security="s_priv"/>
                  <peripheral id="CASPER" security="s_priv"/>
                  <peripheral id="CRC_ENGINE" security="s_priv"/>
                  <peripheral id="CTIMER0" security="s_priv"/>
                  <peripheral id="CTIMER1" security="s_priv"/>
                  <peripheral id="CTIMER2" security="s_priv"/>
                  <peripheral id="CTIMER3" security="s_priv"/>
                  <peripheral id="CTIMER4" security="s_priv"/>
                  <peripheral id="DBGMAILBOX" security="s_priv"/>
                  <peripheral id="DMA0" security="s_priv"/>
                  <peripheral id="DMA1" security="s_priv"/>
                  <peripheral id="FLASH" security="s_priv"/>
                  <peripheral id="FLEXCOMM0" security="s_priv"/>
                  <peripheral id="FLEXCOMM1" security="s_priv"/>
                  <peripheral id="FLEXCOMM2" security="s_priv"/>
                  <peripheral id="FLEXCOMM3" security="s_priv"/>
                  <peripheral id="FLEXCOMM4" security="s_priv"/>
                  <peripheral id="FLEXCOMM5" security="s_priv"/>
                  <peripheral id="FLEXCOMM6" security="s_priv"/>
                  <peripheral id="FLEXCOMM7" security="s_priv"/>
                  <peripheral id="GINT0" security="s_priv"/>
                  <peripheral id="GINT1" security="s_priv"/>
                  <peripheral id="GPIO" security="s_priv"/>
                  <peripheral id="HASHCRYPT" security="s_priv"/>
                  <peripheral id="INPUTMUX" security="s_priv"/>
                  <peripheral id="IOCON" security="s_priv"/>
                  <peripheral id="MAILBOX" security="s_priv"/>
                  <peripheral id="MRT0" security="s_priv"/>
                  <peripheral id="OSTIMER" security="s_priv"/>
                  <peripheral id="PINT" security="s_priv"/>
                  <peripheral id="PLU" security="s_priv"/>
                  <peripheral id="PMC" security="s_priv"/>
                  <peripheral id="POWERQUAD" security="s_priv"/>
                  <peripheral id="PRINCE" security="s_priv"/>
                  <peripheral id="PUF" security="s_priv"/>
                  <peripheral id="RNG" security="s_priv"/>
                  <peripheral id="RTC" security="s_priv"/>
                  <peripheral id="SCT0" security="s_priv"/>
                  <peripheral id="SDIF" security="s_priv"/>
                  <peripheral id="SECGPIO" security="s_priv"/>
                  <peripheral id="SECPINT" security="s_priv"/>
                  <peripheral id="SPI8" security="s_priv"/>
                  <peripheral id="SYSCON" security="s_priv"/>
                  <peripheral id="SYSCTL" security="s_priv"/>
                  <peripheral id="USB0" security="s_priv"/>
                  <peripheral id="USBFSH" security="s_priv"/>
                  <peripheral id="USBHSD" security="s_priv"/>
                  <peripheral id="USBHSH" security="s_priv"/>
                  <peripheral id="USBPHY" security="s_priv"/>
                  <peripheral id="UTICK0" security="s_priv"/>
                  <peripheral id="WWDT" security="s_priv"/>
               </peripherals>
               <interrupts>
                  <masking>
                     <interrupt id="acmp_capt_irq" masked="Masked"/>
                     <interrupt id="adc_irq" masked="Masked"/>
                     <interrupt id="casper_irq" masked="Masked"/>
                     <interrupt id="ctimer0_irq" masked="Masked"/>
                     <interrupt id="ctimer1_irq" masked="Masked"/>
                     <interrupt id="ctimer2_irq" masked="Masked"/>
                     <interrupt id="ctimer3_irq" masked="Masked"/>
                     <interrupt id="ctimer4_irq" masked="Masked"/>
                     <interrupt id="flexcomm0_irq" masked="Masked"/>
                     <interrupt id="flexcomm1_irq" masked="Masked"/>
                     <interrupt id="flexcomm2_irq" masked="Masked"/>
                     <interrupt id="flexcomm3_irq" masked="Masked"/>
                     <interrupt id="flexcomm4_irq" masked="Masked"/>
                     <interrupt id="flexcomm5_irq" masked="Masked"/>
                     <interrupt id="flexcomm6_irq" masked="Masked"/>
                     <interrupt id="flexcomm7_irq" masked="Masked"/>
                     <interrupt id="global_irq0" masked="Masked"/>
                     <interrupt id="global_irq1" masked="Masked"/>
                     <interrupt id="lspi_hs_irq" masked="Masked"/>
                     <interrupt id="mailbox_irq" masked="Masked"/>
                     <interrupt id="mrt_irq" masked="Masked"/>
                     <interrupt id="os_event_irq" masked="Masked"/>
                     <interrupt id="pin_int4" masked="Masked"/>
                     <interrupt id="pin_int5" masked="Masked"/>
                     <interrupt id="pin_int6" masked="Masked"/>
                     <interrupt id="pin_int7" masked="Masked"/>
                     <interrupt id="pin_irq0" masked="Masked"/>
                     <interrupt id="pin_irq1" masked="Masked"/>
                     <interrupt id="pin_irq2" masked="Masked"/>
                     <interrupt id="pin_irq3" masked="Masked"/>
                     <interrupt id="plu_irq" masked="Masked"/>
                     <interrupt id="pq_irq" masked="Masked"/>
                     <interrupt id="qddkey_irq" masked="Masked"/>
                     <interrupt id="rtc_irq" masked="Masked"/>
                     <interrupt id="sct_irq" masked="Masked"/>
                     <interrupt id="sdio_irq" masked="Masked"/>
                     <interrupt id="sdma0_irq" masked="Masked"/>
                     <interrupt id="sdma1_irq" masked="Masked"/>
                     <interrupt id="sec_hypervisor_call_irq" masked="Masked"/>
                     <interrupt id="sec_int0" masked="Masked"/>
                     <interrupt id="sec_int1" masked="Masked"/>
                     <interrupt id="sec_vio_irq" masked="Masked"/>
                     <interrupt id="sha_irq" masked="Masked"/>
                     <interrupt id="sys_irq" masked="Masked"/>
                     <interrupt id="usb0_irq" masked="Masked"/>
                     <interrupt id="usb0_needclk_irq" masked="Masked"/>
                     <interrupt id="usb1_irq" masked="Masked"/>
                     <interrupt id="usb1_needclk_irq" masked="Masked"/>
                     <interrupt id="usb1_utmi_irq" masked="Masked"/>
                     <interrupt id="utick_irq" masked="Masked"/>
                  </masking>
                  <security>
                     <interrupt id="acmp_capt_irq" secure="Secure"/>
                     <interrupt id="adc_irq" secure="Secure"/>
                     <interrupt id="casper_irq" secure="Secure"/>
                     <interrupt id="ctimer0_irq" secure="Secure"/>
                     <interrupt id="ctimer1_irq" secure="Secure"/>
                     <interrupt id="ctimer2_irq" secure="Secure"/>
                     <interrupt id="ctimer3_irq" secure="Secure"/>
                     <interrupt id="ctimer4_irq" secure="Secure"/>
                     <interrupt id="flexcomm0_irq" secure="Secure"/>
                     <interrupt id="flexcomm1_irq" secure="Secure"/>
                     <interrupt id="flexcomm2_irq" secure="Secure"/>
                     <interrupt id="flexcomm3_irq" secure="Secure"/>
                     <interrupt id="flexcomm4_irq" secure="Secure"/>
                     <interrupt id="flexcomm5_irq" secure="Secure"/>
                     <interrupt id="flexcomm6_irq" secure="Secure"/>
                     <interrupt id="flexcomm7_irq" secure="Secure"/>
                     <interrupt id="global_irq0" secure="Secure"/>
                     <interrupt id="global_irq1" secure="Secure"/>
                     <interrupt id="lspi_hs_irq" secure="Secure"/>
                     <interrupt id="mailbox_irq" secure="Secure"/>
                     <interrupt id="mrt_irq" secure="Secure"/>
                     <interrupt id="os_event_irq" secure="Secure"/>
                     <interrupt id="pin_int4" secure="Secure"/>
                     <interrupt id="pin_int5" secure="Secure"/>
                     <interrupt id="pin_int6" secure="Secure"/>
                     <interrupt id="pin_int7" secure="Secure"/>
                     <interrupt id="pin_irq0" secure="Secure"/>
                     <interrupt id="pin_irq1" secure="Secure"/>
                     <interrupt id="pin_irq2" secure="Secure"/>
                     <interrupt id="pin_irq3" secure="Secure"/>
                     <interrupt id="plu_irq" secure="Secure"/>
                     <interrupt id="pq_irq" secure="Secure"/>
                     <interrupt id="qddkey_irq" secure="Secure"/>
                     <interrupt id="rtc_irq" secure="Secure"/>
                     <interrupt id="sct_irq" secure="Secure"/>
                     <interrupt id="sdio_irq" secure="Secure"/>
                     <interrupt id="sdma0_irq" secure="Secure"/>
                     <interrupt id="sdma1_irq" secure="Secure"/>
                     <interrupt id="sec_hypervisor_call_irq" secure="Secure"/>
                     <interrupt id="sec_int0" secure="Secure"/>
                     <interrupt id="sec_int1" secure="Secure"/>
                     <interrupt id="sec_vio_irq" secure="Secure"/>
                     <interrupt id="sha_irq" secure="Secure"/>
                     <interrupt id="sys_irq" secure="Secure"/>
                     <interrupt id="usb0_irq" secure="Secure"/>
                     <interrupt id="usb0_needclk_irq" secure="Secure"/>
                     <interrupt id="usb1_irq" secure="Secure"/>
                     <interrupt id="usb1_needclk_irq" secure="Secure"/>
                     <interrupt id="usb1_utmi_irq" secure="Secure"/>
                     <interrupt id="utick_irq" secure="Secure"/>
                  </security>
               </interrupts>
               <ports>
                  <port id="pio0">
                     <pin_mask id="0" masked="Masked"/>
                     <pin_mask id="1" masked="Masked"/>
                     <pin_mask id="10" masked="Masked"/>
                     <pin_mask id="11" masked="Masked"/>
                     <pin_mask id="12" masked="Masked"/>
                     <pin_mask id="13" masked="Masked"/>
                     <pin_mask id="14" masked="Masked"/>
                     <pin_mask id="15" masked="Masked"/>
                     <pin_mask id="16" masked="Masked"/>
                     <pin_mask id="17" masked="Masked"/>
                     <pin_mask id="18" masked="Masked"/>
                     <pin_mask id="19" masked="Masked"/>
                     <pin_mask id="2" masked="Masked"/>
                     <pin_mask id="20" masked="Masked"/>
                     <pin_mask id="21" masked="Masked"/>
                     <pin_mask id="22" masked="Masked"/>
                     <pin_mask id="23" masked="Masked"/>
                     <pin_mask id="24" masked="Masked"/>
                     <pin_mask id="25" masked="Masked"/>
                     <pin_mask id="26" masked="Masked"/>
                     <pin_mask id="27" masked="Masked"/>
                     <pin_mask id="28" masked="Masked"/>
                     <pin_mask id="29" masked="Masked"/>
                     <pin_mask id="3" masked="Masked"/>
                     <pin_mask id="30" masked="Masked"/>
                     <pin_mask id="31" masked="Masked"/>
                     <pin_mask id="4" masked="Masked"/>
                     <pin_mask id="5" masked="Masked"/>
                     <pin_mask id="6" masked="Masked"/>
                     <pin_mask id="7" masked="Masked"/>
                     <pin_mask id="8" masked="Masked"/>
                     <pin_mask id="9" masked="Masked"/>
                  </port>
                  <port id="pio1">
                     <pin_mask id="0" masked="Masked"/>
                     <pin_mask id="1" masked="Masked"/>
                     <pin_mask id="10" masked="Masked"/>
                     <pin_mask id="11" masked="Masked"/>
                     <pin_mask id="12" masked="Masked"/>
                     <pin_mask id="13" masked="Masked"/>
                     <pin_mask id="14" masked="Masked"/>
                     <pin_mask id="15" masked="Masked"/>
                     <pin_mask id="16" masked="Masked"/>
                     <pin_mask id="17" masked="Masked"/>
                     <pin_mask id="18" masked="Masked"/>
                     <pin_mask id="19" masked="Masked"/>
                     <pin_mask id="2" masked="Masked"/>
                     <pin_mask id="20" masked="Masked"/>
                     <pin_mask id="21" masked="Masked"/>
                     <pin_mask id="22" masked="Masked"/>
                     <pin_mask id="23" masked="Masked"/>
                     <pin_mask id="24" masked="Masked"/>
                     <pin_mask id="25" masked="Masked"/>
                     <pin_mask id="26" masked="Masked"/>
                     <pin_mask id="27" masked="Masked"/>
                     <pin_mask id="28" masked="Masked"/>
                     <pin_mask id="29" masked="Masked"/>
                     <pin_mask id="3" masked="Masked"/>
                     <pin_mask id="30" masked="Masked"/>
                     <pin_mask id="31" masked="Masked"/>
                     <pin_mask id="4" masked="Masked"/>
                     <pin_mask id="5" masked="Masked"/>
                     <pin_mask id="6" masked="Masked"/>
                     <pin_mask id="7" masked="Masked"/>
                     <pin_mask id="8" masked="Masked"/>
                     <pin_mask id="9" masked="Masked"/>
                  </port>
               </ports>
            </ahb>
            <saus>
               <sau enabled="true" all_non_secure="false" generate_code_for_disabled_regions="false">
                  <region start="0" size="268435456" security="ns" enabled="true" index="0"/>
                  <region start="536870912" size="3221225472" security="ns" enabled="true" index="1"/>
                  <region start="0" size="32" security="ns" enabled="false" index="2"/>
                  <region start="0" size="32" security="ns" enabled="false" index="3"/>
                  <region start="0" size="32" security="ns" enabled="false" index="4"/>
                  <region start="0" size="32" security="ns" enabled="false" index="5"/>
                  <region start="0" size="32" security="ns" enabled="false" index="6"/>
                  <region start="0" size="32" security="ns" enabled="false" index="7"/>
               </sau>
            </saus>
            <global_options>
               <option id="AIRCR_PRIS" value="no"/>
               <option id="AIRCR_BFHFNMINS" value="no"/>
               <option id="AIRCR_SYSRESETREQS" value="no"/>
               <option id="SCR_SLEEPDEEPS" value="no"/>
               <option id="SHCSR_SECUREFAULTENA" value="no"/>
               <option id="CPACR_CP0" value="3"/>
               <option id="CPACR_CP1" value="3"/>
               <option id="CPACR_CP2" value="0"/>
               <option id="CPACR_CP3" value="0"/>
               <option id="CPACR_CP4" value="0"/>
               <option id="CPACR_CP5" value="0"/>
               <option id="CPACR_CP6" value="0"/>
               <option id="CPACR_CP7" value="0"/>
               <option id="CPACR_CP10" value="3"/>
               <option id="CPACR_CP11" value="3"/>
               <option id="NSACR_CP0" value="yes"/>
               <option id="NSACR_CP1" value="yes"/>
               <option id="NSACR_CP2" value="no"/>
               <option id="NSACR_CP3" value="no"/>
               <option id="NSACR_CP4" value="no"/>
               <option id="NSACR_CP5" value="no"/>
               <option id="NSACR_CP6" value="no"/>
               <option id="NSACR_CP7" value="no"/>
               <option id="NSACR_CP10" value="yes"/>
               <option id="NSACR_CP11" value="yes"/>
               <option id="CPPWR_SU0" value="no"/>
               <option id="CPPWR_SUS0" value="no"/>
               <option id="CPPWR_SU1" value="no"/>
               <option id="CPPWR_SUS1" value="no"/>
               <option id="CPPWR_SU2" value="no"/>
               <option id="CPPWR_SUS2" value="no"/>
               <option id="CPPWR_SU3" value="no"/>
               <option id="CPPWR_SUS3" value="no"/>
               <option id="CPPWR_SU4" value="no"/>
               <option id="CPPWR_SUS4" value="no"/>
               <option id="CPPWR_SU5" value="no"/>
               <option id="CPPWR_SUS5" value="no"/>
               <option id="CPPWR_SU6" value="no"/>
               <option id="CPPWR_SUS6" value="no"/>
               <option id="CPPWR_SU7" value="no"/>
               <option id="CPPWR_SUS7" value="no"/>
               <option id="CPPWR_SU10" value="no"/>
               <option id="CPPWR_SUS10" value="no"/>
               <option id="CPPWR_SU11" value="no"/>
               <option id="CPPWR_SUS11" value="no"/>
               <option id="SEC_GPIO_MASK0_LOCK" value="no"/>
               <option id="SEC_GPIO_MASK1_LOCK" value="no"/>
               <option id="SEC_CPU1_INT_MASK0_LOCK" value="no"/>
               <option id="SEC_CPU1_INT_MASK1_LOCK" value="no"/>
               <option id="MASTER_SEC_LEVEL_LOCK" value="no"/>
               <option id="CPU0_LOCK_NS_VTOR" value="no"/>
               <option id="CPU0_LOCK_NS_MPU" value="no"/>
               <option id="CPU0_LOCK_S_VTAIRCR" value="no"/>
               <option id="CPU0_LOCK_S_MPU" value="no"/>
               <option id="CPU0_LOCK_SAU" value="no"/>
               <option id="CPU0_LOCK_REG_LOCK" value="no"/>
               <option id="CPU1_LOCK_NS_VTOR" value="no"/>
               <option id="CPU1_LOCK_NS_MPU" value="no"/>
               <option id="CPU1_LOCK_REG_LOCK" value="no"/>
               <option id="AHB_MISC_CTRL_REG_ENABLE_SECURE_CHECKING" value="yes"/>
               <option id="AHB_MISC_CTRL_REG_ENABLE_S_PRIV_CHECK" value="yes"/>
               <option id="AHB_MISC_CTRL_REG_ENABLE_NS_PRIV_CHECK" value="yes"/>
               <option id="AHB_MISC_CTRL_REG_DISABLE_VIOLATION_ABORT" value="no"/>
               <option id="AHB_MISC_CTRL_REG_DISABLE_SIMPLE_MASTER_STRICT_MODE" value="no"/>
               <option id="AHB_MISC_CTRL_REG_DISABLE_SMART_MASTER_STRICT_MODE" value="no"/>
               <option id="AHB_MISC_CTRL_REG_IDAU_ALL_NS" value="no"/>
               <option id="AHB_MISC_CTRL_REG_WRITE_LOCK" value="yes"/>
            </global_options>
            <mpus>
               <mpu enabled="false" priv_default_map="false" handler_enabled="false" id="s" generate_code_for_disabled_regions="false">
                  <attributes>
                     <group index="0" id="Code" memory_type="normal" device="nGnRE"/>
                     <group index="1" id="RAM" memory_type="normal" device="nGnRE"/>
                     <group index="2" id="Peripheral" memory_type="device" device="nGnRE"/>
                     <group index="3" id="3" memory_type="device" device="nGnRE"/>
                     <group index="4" id="4" memory_type="device" device="nGnRE"/>
                     <group index="5" id="5" memory_type="device" device="nGnRE"/>
                     <group index="6" id="6" memory_type="device" device="nGnRE"/>
                     <group index="7" id="7" memory_type="device" device="nGnRE"/>
                  </attributes>
                  <regions>
                     <region start="0" size="32" security="priv" enabled="false" index="0" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="1" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="2" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="3" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="4" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="5" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="6" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="7" executable="false" read_only="false" attributes_index="0"/>
                  </regions>
               </mpu>
               <mpu enabled="false" priv_default_map="false" handler_enabled="false" id="ns" generate_code_for_disabled_regions="false">
                  <attributes>
                     <group index="0" id="Code" memory_type="normal" device="nGnRE"/>
                     <group index="1" id="RAM" memory_type="normal" device="nGnRE"/>
                     <group index="2" id="Peripheral" memory_type="device" device="nGnRE"/>
                     <group index="3" id="3" memory_type="device" device="nGnRE"/>
                     <group index="4" id="4" memory_type="device" device="nGnRE"/>
                     <group index="5" id="5" memory_type="device" device="nGnRE"/>
                     <group index="6" id="6" memory_type="device" device="nGnRE"/>
                     <group index="7" id="7" memory_type="device" device="nGnRE"/>
                  </attributes>
                  <regions>
                     <region start="0" size="32" security="priv" enabled="false" index="0" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="1" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="2" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="3" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="4" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="5" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="6" executable="false" read_only="false" attributes_index="0"/>
                     <region start="0" size="32" security="priv" enabled="false" index="7" executable="false" read_only="false" attributes_index="0"/>
                  </regions>
               </mpu>
            </mpus>
         </functional_group>
      </tee>
   </tools>
</configuration>
