;************************************************************
; Windows USB CDC ACM Setup File
; Copyright (c) 2000 Microsoft Corporation


[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MFGNAME%
LayoutFile=layout.inf
CatalogFile=%MFGFILENAME%.cat
DriverVer=11/15/2007,5.1.2600.0
DriverPackageDisplayName=%DESCRIPTION%

[Manufacturer]
%MFGNAME%=DeviceList, NTamd64

[DestinationDirs]
DefaultDestDir=12


;------------------------------------------------------------------------------
;  Windows 2000/XP/Vista-32bit Sections
;------------------------------------------------------------------------------

[DriverInstall.nt]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.nt
AddReg=DriverInstall.nt.AddReg

[DriverCopyFiles.nt]
usbser.sys,,,0x20

[DriverInstall.nt.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,%DRIVERFILENAME%.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.nt.Services]
AddService=usbser, 0x00000002, DriverService.nt

[DriverService.nt]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\%DRIVERFILENAME%.sys

;------------------------------------------------------------------------------
;  Vista-64bit Sections
;------------------------------------------------------------------------------

[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.NTamd64
AddReg=DriverInstall.NTamd64.AddReg

[DriverCopyFiles.NTamd64]
%DRIVERFILENAME%.sys,,,0x20

[DriverInstall.NTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,%DRIVERFILENAME%.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverService.NTamd64

[DriverService.NTamd64]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\%DRIVERFILENAME%.sys


;------------------------------------------------------------------------------
;  Vendor and Product ID Definitions
;------------------------------------------------------------------------------
; When developing your USB device, the VID and PID used in the PC side
; application program and the firmware on the microcontroller must match.
; Modify the below line to use your VID and PID.  Use the format as shown below.
; Note: One INF file can be used for multiple devices with different VID and PIDs.
; For each supported device, append ",USB\VID_xxxx&PID_yyyy" to the end of the line.
;------------------------------------------------------------------------------
[SourceDisksFiles]
[SourceDisksNames]
[DeviceList]

%DESCRIPTION%=DriverInstall, USB\VID_CAFE&PID_4001&MI_00, USB\VID_CAFE&PID_4003&MI_00, USB\VID_CAFE&PID_4005&MI_00, USB\VID_CAFE&PID_4007&MI_00, USB\VID_CAFE&PID_4009&MI_00, USB\VID_CAFE&PID_400b&MI_00, USB\VID_CAFE&PID_400d&MI_00, USB\VID_CAFE&PID_400f&MI_00, USB\VID_CAFE&PID_4011&MI_00, USB\VID_CAFE&PID_4013&MI_00, USB\VID_CAFE&PID_4015&MI_00, USB\VID_CAFE&PID_4017&MI_00, USB\VID_CAFE&PID_4019&MI_00, USB\VID_CAFE&PID_401b&MI_00, USB\VID_CAFE&PID_401d&MI_00, USB\VID_CAFE&PID_401f&MI_00, USB\VID_CAFE&PID_4021&MI_00, USB\VID_CAFE&PID_4023&MI_00, USB\VID_CAFE&PID_4025&MI_00, USB\VID_CAFE&PID_4027&MI_00, USB\VID_CAFE&PID_4029&MI_00, USB\VID_CAFE&PID_402b&MI_00, USB\VID_CAFE&PID_402d&MI_00, USB\VID_CAFE&PID_402f&MI_00, USB\VID_CAFE&PID_4031&MI_00, USB\VID_CAFE&PID_4033&MI_00, USB\VID_CAFE&PID_4035&MI_00, USB\VID_CAFE&PID_4037&MI_00, USB\VID_CAFE&PID_4039&MI_00, USB\VID_CAFE&PID_403b&MI_00, USB\VID_CAFE&PID_403d&MI_00, USB\VID_CAFE&PID_403f&MI_00


[DeviceList.NTamd64]
%DESCRIPTION%=DriverInstall, USB\VID_CAFE&PID_4001&MI_00, USB\VID_CAFE&PID_4003&MI_00, USB\VID_CAFE&PID_4005&MI_00, USB\VID_CAFE&PID_4007&MI_00, USB\VID_CAFE&PID_4009&MI_00, USB\VID_CAFE&PID_400b&MI_00, USB\VID_CAFE&PID_400d&MI_00, USB\VID_CAFE&PID_400f&MI_00, USB\VID_CAFE&PID_4011&MI_00, USB\VID_CAFE&PID_4013&MI_00, USB\VID_CAFE&PID_4015&MI_00, USB\VID_CAFE&PID_4017&MI_00, USB\VID_CAFE&PID_4019&MI_00, USB\VID_CAFE&PID_401b&MI_00, USB\VID_CAFE&PID_401d&MI_00, USB\VID_CAFE&PID_401f&MI_00, USB\VID_CAFE&PID_4021&MI_00, USB\VID_CAFE&PID_4023&MI_00, USB\VID_CAFE&PID_4025&MI_00, USB\VID_CAFE&PID_4027&MI_00, USB\VID_CAFE&PID_4029&MI_00, USB\VID_CAFE&PID_402b&MI_00, USB\VID_CAFE&PID_402d&MI_00, USB\VID_CAFE&PID_402f&MI_00, USB\VID_CAFE&PID_4031&MI_00, USB\VID_CAFE&PID_4033&MI_00, USB\VID_CAFE&PID_4035&MI_00, USB\VID_CAFE&PID_4037&MI_00, USB\VID_CAFE&PID_4039&MI_00, USB\VID_CAFE&PID_403b&MI_00, USB\VID_CAFE&PID_403d&MI_00, USB\VID_CAFE&PID_403f&MI_00

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------
;Modify these strings to customize your device
;------------------------------------------------------------------------------
[Strings]
MFGFILENAME="tinyusb_usbser"
DRIVERFILENAME ="usbser"
MFGNAME="tinyusb.org"
INSTDISK="tinyusb CDC Driver"
DESCRIPTION="tinyusb Serial"
SERVICE="USB RS-232 Emulation Driver"
