<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="MIMXRT1024-EVK" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_13 http://mcuxpresso.nxp.com/XSD/mex_configuration_13.xsd" uuid="a558cc6e-82c2-41f9-9f55-0348efc7896f" version="13" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_13" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MIMXRT1024xxxxx</processor>
      <package>MIMXRT1024DAG5A</package>
      <board>MIMXRT1024-EVK</board>
      <board_revision>B1</board_revision>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M7F" id="core0" description="M7 core"/>
      </cores>
      <description></description>
   </common>
   <preferences>
      <validate_boot_init_only>false</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <update_include_paths>true</update_include_paths>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="13.1" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>13.0.2</processor_version>
            <pin_labels>
               <pin_label pin_num="52" pin_signal="WAKEUP" label="USER_BUTTON" identifier="USER_BUTTON"/>
               <pin_label pin_num="82" pin_signal="GPIO_AD_B1_08" label="UART_TX/USER_LED/J17[4]" identifier="USER_LED"/>
            </pin_labels>
            <power_domains>
               <power_domain name="NVCC_GPIO" value="3.3"/>
            </power_domains>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="GPIO5" description="Peripheral GPIO5 is not initialized" problem_level="1" source="Pins:BOARD_InitPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Pins initialization requires the IGPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIO5" signal="gpio_io, 00" pin_num="52" pin_signal="WAKEUP">
                     <pin_features>
                        <pin_feature name="direction" value="INPUT"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO1" signal="gpio_io, 24" pin_num="82" pin_signal="GPIO_AD_B1_08">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitDEBUG_UARTPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="LPUART1" description="Peripheral LPUART1 is not initialized" problem_level="1" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="LPUART1" signal="RX" pin_num="101" pin_signal="GPIO_AD_B0_07"/>
                  <pin peripheral="LPUART1" signal="TX" pin_num="105" pin_signal="GPIO_AD_B0_06"/>
               </pins>
            </function>
            <function name="BOARD_InitSDRAMPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="SEMC" description="Peripheral SEMC is not initialized" problem_level="1" source="Pins:BOARD_InitSDRAMPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitSDRAMPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitSDRAMPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="SEMC" signal="ADDR, 00" pin_num="142" pin_signal="GPIO_EMC_16"/>
                  <pin peripheral="SEMC" signal="ADDR, 01" pin_num="141" pin_signal="GPIO_EMC_17"/>
                  <pin peripheral="SEMC" signal="ADDR, 02" pin_num="140" pin_signal="GPIO_EMC_18"/>
                  <pin peripheral="SEMC" signal="ADDR, 03" pin_num="139" pin_signal="GPIO_EMC_19"/>
                  <pin peripheral="SEMC" signal="ADDR, 04" pin_num="138" pin_signal="GPIO_EMC_20"/>
                  <pin peripheral="SEMC" signal="ADDR, 06" pin_num="136" pin_signal="GPIO_EMC_22"/>
                  <pin peripheral="SEMC" signal="ADDR, 05" pin_num="137" pin_signal="GPIO_EMC_21"/>
                  <pin peripheral="SEMC" signal="ADDR, 07" pin_num="133" pin_signal="GPIO_EMC_23"/>
                  <pin peripheral="SEMC" signal="ADDR, 08" pin_num="132" pin_signal="GPIO_EMC_24"/>
                  <pin peripheral="SEMC" signal="ADDR, 09" pin_num="131" pin_signal="GPIO_EMC_25"/>
                  <pin peripheral="SEMC" signal="ADDR, 10" pin_num="143" pin_signal="GPIO_EMC_15"/>
                  <pin peripheral="SEMC" signal="ADDR, 11" pin_num="130" pin_signal="GPIO_EMC_26"/>
                  <pin peripheral="SEMC" signal="ADDR, 12" pin_num="129" pin_signal="GPIO_EMC_27"/>
                  <pin peripheral="SEMC" signal="BA, 0" pin_num="2" pin_signal="GPIO_EMC_13"/>
                  <pin peripheral="SEMC" signal="BA, 1" pin_num="1" pin_signal="GPIO_EMC_14"/>
                  <pin peripheral="SEMC" signal="semc_cas" pin_num="7" pin_signal="GPIO_EMC_10"/>
                  <pin peripheral="SEMC" signal="semc_cke" pin_num="127" pin_signal="GPIO_EMC_29"/>
                  <pin peripheral="SEMC" signal="semc_clk" pin_num="126" pin_signal="GPIO_EMC_30"/>
                  <pin peripheral="SEMC" signal="CS, 0" pin_num="3" pin_signal="GPIO_EMC_12"/>
                  <pin peripheral="SEMC" signal="semc_we" pin_num="8" pin_signal="GPIO_EMC_09"/>
                  <pin peripheral="SEMC" signal="semc_ras" pin_num="4" pin_signal="GPIO_EMC_11"/>
                  <pin peripheral="SEMC" signal="semc_dqs" pin_num="128" pin_signal="GPIO_EMC_28"/>
                  <pin peripheral="SEMC" signal="DM, 1" pin_num="125" pin_signal="GPIO_EMC_31"/>
                  <pin peripheral="SEMC" signal="DM, 0" pin_num="9" pin_signal="GPIO_EMC_08"/>
                  <pin peripheral="SEMC" signal="DATA, 15" pin_num="117" pin_signal="GPIO_EMC_39"/>
                  <pin peripheral="SEMC" signal="DATA, 14" pin_num="118" pin_signal="GPIO_EMC_38"/>
                  <pin peripheral="SEMC" signal="DATA, 13" pin_num="119" pin_signal="GPIO_EMC_37"/>
                  <pin peripheral="SEMC" signal="DATA, 12" pin_num="120" pin_signal="GPIO_EMC_36"/>
                  <pin peripheral="SEMC" signal="DATA, 10" pin_num="122" pin_signal="GPIO_EMC_34"/>
                  <pin peripheral="SEMC" signal="DATA, 11" pin_num="121" pin_signal="GPIO_EMC_35"/>
                  <pin peripheral="SEMC" signal="DATA, 09" pin_num="123" pin_signal="GPIO_EMC_33"/>
                  <pin peripheral="SEMC" signal="DATA, 08" pin_num="124" pin_signal="GPIO_EMC_32"/>
                  <pin peripheral="SEMC" signal="DATA, 07" pin_num="10" pin_signal="GPIO_EMC_07"/>
                  <pin peripheral="SEMC" signal="DATA, 06" pin_num="12" pin_signal="GPIO_EMC_06"/>
                  <pin peripheral="SEMC" signal="DATA, 05" pin_num="13" pin_signal="GPIO_EMC_05"/>
                  <pin peripheral="SEMC" signal="DATA, 04" pin_num="14" pin_signal="GPIO_EMC_04"/>
                  <pin peripheral="SEMC" signal="DATA, 03" pin_num="15" pin_signal="GPIO_EMC_03"/>
                  <pin peripheral="SEMC" signal="DATA, 02" pin_num="16" pin_signal="GPIO_EMC_02"/>
                  <pin peripheral="SEMC" signal="DATA, 01" pin_num="17" pin_signal="GPIO_EMC_01"/>
                  <pin peripheral="SEMC" signal="DATA, 00" pin_num="18" pin_signal="GPIO_EMC_00"/>
               </pins>
            </function>
            <function name="BOARD_InitCANPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="CAN1" description="Peripheral CAN1 is not initialized" problem_level="1" source="Pins:BOARD_InitCANPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitCANPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitCANPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="CAN1" signal="RX" pin_num="32" pin_signal="GPIO_SD_B1_01"/>
                  <pin peripheral="CAN1" signal="TX" pin_num="33" pin_signal="GPIO_SD_B1_00"/>
               </pins>
            </function>
            <function name="BOARD_InitENETPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="ENET" description="Peripheral ENET is not initialized" problem_level="1" source="Pins:BOARD_InitENETPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitENETPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitENETPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="ENET" signal="enet_rx_en" pin_num="97" pin_signal="GPIO_AD_B0_11"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 22" pin_num="84" pin_signal="GPIO_AD_B1_06"/>
                  <pin peripheral="GPIO1" signal="gpio_io, 04" pin_num="107" pin_signal="GPIO_AD_B0_04"/>
                  <pin peripheral="ENET" signal="enet_tx_clk" pin_num="100" pin_signal="GPIO_AD_B0_08"/>
                  <pin peripheral="ENET" signal="enet_tx_en" pin_num="95" pin_signal="GPIO_AD_B0_13"/>
                  <pin peripheral="ENET" signal="enet_tx_data, 1" pin_num="93" pin_signal="GPIO_AD_B0_15"/>
                  <pin peripheral="ENET" signal="enet_tx_data, 0" pin_num="94" pin_signal="GPIO_AD_B0_14"/>
                  <pin peripheral="ENET" signal="enet_rx_er" pin_num="96" pin_signal="GPIO_AD_B0_12"/>
                  <pin peripheral="ENET" signal="enet_rx_data, 1" pin_num="99" pin_signal="GPIO_AD_B0_09"/>
                  <pin peripheral="ENET" signal="enet_rx_data, 0" pin_num="98" pin_signal="GPIO_AD_B0_10"/>
                  <pin peripheral="ENET" signal="enet_mdio" pin_num="116" pin_signal="GPIO_EMC_40"/>
                  <pin peripheral="ENET" signal="enet_mdc" pin_num="115" pin_signal="GPIO_EMC_41"/>
               </pins>
            </function>
            <function name="BOARD_InitUSDHCPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="USDHC1" description="Peripheral USDHC1 is not initialized" problem_level="1" source="Pins:BOARD_InitUSDHCPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitUSDHCPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitUSDHCPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="USDHC1" signal="usdhc_clk" pin_num="45" pin_signal="GPIO_SD_B0_03"/>
                  <pin peripheral="USDHC1" signal="usdhc_cmd" pin_num="46" pin_signal="GPIO_SD_B0_02"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 0" pin_num="43" pin_signal="GPIO_SD_B0_04"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 1" pin_num="42" pin_signal="GPIO_SD_B0_05"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 2" pin_num="48" pin_signal="GPIO_SD_B0_00"/>
                  <pin peripheral="USDHC1" signal="usdhc_data, 3" pin_num="47" pin_signal="GPIO_SD_B0_01"/>
                  <pin peripheral="GPIO3" signal="gpio_io, 19" pin_num="41" pin_signal="GPIO_SD_B0_06"/>
               </pins>
            </function>
            <function name="BOARD_InitQSPIPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="FLEXSPI" description="Peripheral FLEXSPI is not initialized" problem_level="1" source="Pins:BOARD_InitQSPIPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitQSPIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitQSPIPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_SCLK" pin_num="24" pin_signal="GPIO_SD_B1_07"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA0" pin_num="23" pin_signal="GPIO_SD_B1_08"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA1" pin_num="21" pin_signal="GPIO_SD_B1_10"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA2" pin_num="22" pin_signal="GPIO_SD_B1_09"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_DATA3" pin_num="25" pin_signal="GPIO_SD_B1_06"/>
                  <pin peripheral="FLEXSPI" signal="FLEXSPI_A_SS0_B" pin_num="19" pin_signal="GPIO_SD_B1_11"/>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="11.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>13.0.2</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: XTALOSC24M.rtc_xtali, Clocks tool id: XTALOSC24M.RTC_XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: XTALOSC24M.rtc_xtali, Clocks tool id: XTALOSC24M.RTC_XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: XTALOSC24M.rtc_xtalo, Clocks tool id: XTALOSC24M.RTC_XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: XTALOSC24M.rtc_xtalo, Clocks tool id: XTALOSC24M.RTC_XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtali" description="&apos;XTALI&apos; (Pins tool id: XTALOSC24M.xtali, Clocks tool id: XTALOSC24M.XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="XTALOSC24M.xtalo" description="&apos;XTALO&apos; (Pins tool id: XTALOSC24M.xtalo, Clocks tool id: XTALOSC24M.XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Clocks initialization requires the IOMUXC Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="XTALOSC24M.RTC_OSC.outFreq" value="32.768 kHz" locked="false" enabled="true"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="AHB_CLK_ROOT.outFreq" value="500 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN_CLK_ROOT.outFreq" value="40 MHz" locked="false" accuracy=""/>
                  <clock_output id="CKIL_SYNC_CLK_ROOT.outFreq" value="32.768 kHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_1M.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_24M.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_500M_REF_CLK.outFreq" value="500 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO1_CLK_ROOT.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_ipg_clk_highfreq.outFreq" value="62.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_ipg_clk_highfreq.outFreq" value="62.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="IPG_CLK_ROOT.outFreq" value="125 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C_CLK_ROOT.outFreq" value="60 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI_CLK_ROOT.outFreq" value="105.6 MHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_MCLK.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="PERCLK_CLK_ROOT.outFreq" value="62.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK2.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_CLK_ROOT.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK1.outFreq" value="1080/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK3.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="SEMC_CLK_ROOT.outFreq" value="62.5 MHz" locked="false" accuracy=""/>
                  <clock_output id="SPDIF0_CLK_ROOT.outFreq" value="30 MHz" locked="false" accuracy=""/>
                  <clock_output id="TRACE_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="UART_CLK_ROOT.outFreq" value="80 MHz" locked="false" accuracy=""/>
                  <clock_output id="USBPHY1_CLK.outFreq" value="480 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC1_CLK_ROOT.outFreq" value="176 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC2_CLK_ROOT.outFreq" value="176 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="CCM.AHB_PODF.scale" value="1" locked="true"/>
                  <setting id="CCM.ARM_PODF.scale" value="1" locked="true"/>
                  <setting id="CCM.FLEXSPI_PODF.scale" value="4" locked="true"/>
                  <setting id="CCM.FLEXSPI_SEL.sel" value="CCM_ANALOG.PLL2_PFD2_CLK" locked="false"/>
                  <setting id="CCM.IPG_PODF.scale" value="4" locked="false"/>
                  <setting id="CCM.LPSPI_PODF.scale" value="5" locked="true"/>
                  <setting id="CCM.PERCLK_PODF.scale" value="2" locked="true"/>
                  <setting id="CCM.PRE_PERIPH_CLK_SEL.sel" value="CCM.ARM_PODF" locked="false"/>
                  <setting id="CCM.SEMC_PODF.scale" value="8" locked="false"/>
                  <setting id="CCM.TRACE_CLK_SEL.sel" value="CCM_ANALOG.PLL2_MAIN_CLK" locked="false"/>
                  <setting id="CCM.TRACE_PODF.scale" value="4" locked="true"/>
                  <setting id="CCM.USDHC1_PODF.scale" value="3" locked="true"/>
                  <setting id="CCM.USDHC2_PODF.scale" value="3" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.denom" value="1" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2.num" value="0" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_BYPASS.sel" value="CCM_ANALOG.PLL2_OUT_CLK" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_DIV.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_PFD2_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL2_PFD3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_DIV.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL2_PFD3_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_BYPASS.sel" value="CCM_ANALOG.PLL3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD0" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_DIV.scale" value="22" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD0_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD1_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD1" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD2_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD2" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD3_BYPASS.sel" value="CCM_ANALOG.PLL3_PFD3" locked="false"/>
                  <setting id="CCM_ANALOG.PLL3_PFD3_DIV.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL3_PFD3_MUL.scale" value="18" locked="true"/>
                  <setting id="CCM_ANALOG.PLL4.denom" value="50" locked="false"/>
                  <setting id="CCM_ANALOG.PLL4.div" value="47" locked="false"/>
                  <setting id="CCM_ANALOG.PLL6_BYPASS.sel" value="CCM_ANALOG.PLL6" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_ENET_ENABLE_CFG" value="Disabled" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_ENET_ENET_25M_REF_EN_CFG" value="Disabled" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_USB1_EN_USB_CLKS_CFG" value="Enabled" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_USB1_EN_USB_CLKS_OUT_CFG" value="Enabled" locked="false"/>
                  <setting id="CCM_ANALOG_PLL_USB1_POWER_CFG" value="Yes" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="3.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <dcdx_profile>
            <processor_version>13.0.2</processor_version>
            <output_format>c_array</output_format>
         </dcdx_profile>
         <dcdx_configurations>
            <dcdx_configuration name="Device_configuration">
               <description></description>
               <options/>
               <command_groups/>
            </dcdx_configuration>
         </dcdx_configurations>
      </dcdx>
      <periphs name="Peripherals" version="12.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <peripherals_profile>
            <processor_version>13.0.2</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="6d394465-bc9b-47f2-9a1f-3ca61f76d27b" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies/>
               <instances>
                  <instance name="NVIC" uuid="096e7e36-6917-481a-a4c5-06822cfc2da4" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="5dc935cc-5865-4d50-bac9-89ad440a12ee" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="msg" uuid="c2fe99b8-bf9b-437f-9446-a35000b06679" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
            <component name="generic_uart" uuid="eca93ea1-cadf-4247-bfdc-08769ef8ed12" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="generic_can" uuid="fdf82c69-a73f-4f32-9699-457260453bc6" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
            <component name="gpio_adapter_common" uuid="af80d7a8-d163-4a6f-839d-0ce2b15abffd" type_id="gpio_adapter_common_57579b9ac814fe26bf95df0a384c36b6">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
            <component name="uart_cmsis_common" uuid="dca6ee55-a78d-4884-99bd-4f821b552213" type_id="uart_cmsis_common_9cb8e302497aa696fdbb5a4fd622c2a8">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="generic_enet" uuid="4c34638b-b184-4e9d-8a81-5f3a1287180a" type_id="generic_enet_74db5c914f0ddbe47d86af40cb77a619">
               <config_set_global name="global_enet"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="4.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
      </tee>
      <common name="common" version="1.0" enabled="true" update_project_code="true">
         <core name="core0" role="primary" project_name="Project"/>
      </common>
   </tools>
</configuration>
